# Connext API Datapoints

Data points stored by default in the cloud and available in APIs as of Connext version 915.03.0.

Datapoint | ID hexadecimal | Category | Description | Unit | Section
GEWASTEMP.GEM_GEWAS | D0 | MEAS BOX | plant temperature | °C | I100 Measured plant temperature at this moment. M105 The measured plant temperature. M105.1 The measured plant temperature.
GEWASTEMP.GEWAS_RV | D2 | MEAS BOX | relative humidity | % | M105 The calculated relative air humidity at the measured plant temperature. M105.1 The relative air humidity for the measured plant temperature.
GEWASTEMP.GEWAS_VD | D3 | MEAS BOX | humidity deficit | g/m³ | M105 The calculated humidity deficit for the measured plant temperature. M105.1 The humidity deficit for the measured plant temperature.
GEWASTEMP.GEWAS_VPD | D4 | MEAS BOX | VPD | kPa | M105 The calculated vapour pressure deficit for the measured plant temperature. The vapour pressure deficit is the difference between the vapour pressure in the crop's stomata and the vapour pressure in the greenhouse air. M105.1 The calculated vapour pressure deficit for the measured plant temperature.
KASLBOX.AV_KAS | 104 | MEAS BOX | absolute humidity | g/m³ | I100 Measured relative humidity or humidity deficit at this moment. M105 The absolute humidity. M105.1 The absolute humidity.
KASLBOX.DAUWPUNT_KAS | 10E | MEAS BOX | Dew point | °C | M105 The calculated temperature whereby the humidity from the air condenses. If part of the plant is below this temperature, it will become 'become wet'. M105.1 The calculated temperature whereby the humidity from the air condenses. If part of the plant is below this temperature, it will become 'become wet'.
KASLBOX.GEM_CO2 | 10F | MEAS BOX | CO₂ | ppm | M105 The measured CO2 concentration. M105.1 The measured CO2 concentration.
KASLBOX.GEM_KAS_RV | 110 | MEAS BOX | relative humidity | % | I100 Measured relative humidity or humidity deficit at this moment. M105 The relative air humidity. M105.1 The relative air humidity.
KASLBOX.GEM_KAS_VD | 111 | MEAS BOX | humidity deficit | g/m³ | I100 Measured relative humidity or humidity deficit at this moment. M105 The humidity deficit. M105.1 The humidity deficit.
KASLBOX.GEM_KASNBOL | 112 | MEAS BOX | Wet bulb temperature | °C | M105 The wet bulb temperature. M105.1 The measured wet bulb temperature.
KASLBOX.GEM_KASTEMP | 113 | MEAS BOX | temperature | °C | I100 The measured greenhouse temperature that is passed on to the controls. M105 The dry bulb temperature, so the greenhouse temperature. M105.1 The measured greenhouse temperature that is passed on to the controls.
KASLBOX.MeasEnthalpy | 5DA0 | MEAS BOX | Enthalpy | kJ/kg | M105 The measured enthalpy of the greenhouse air.
KASLBOX.PLANT_TEMP | 127 | MEAS BOX | temperature | °C | M105 The calculated temperature of the plant, stems and fruit in the shadow. M105.1 The calculated temperature of the plant, stems and fruit in the shadow.
KASLBOX.RUWE_KASTEMP | 12C | MEAS BOX | greenhouse temperature | °C | M105.1 The measured greenhouse temperature at this moment.
CPOMPSYS.GER_POMP_CAP | 148 | MOD COOL | Act pump capacity | % | I222 Actual pump capacity of the modulating cooling system.
CPOMPSYS.POMP_STATE | 14C | MOD COOL | Pump status 0=OFF 1=ANTI STUCK PROT. 2=DELAY OFF 3=ON 4=SWITCH DELAY 5=HIGH SP |  | I222 Indication of the pump(s) in the cooling system.
MKOEL_IO.GEM_KOELW_TEMP | 163 | MOD COOL | Meas cooling water temperature | °C | I222 Measured temperature of the cooling water in the cooling system.
MOD_KOELS.BER_KOELW_TEMP | 165 | MOD COOL | Calc cooling water temperature | °C | I222 Calculated temperature of the cooling water of the cooling system.
VDC_STU.TOESTAND | 1C1 | PAD PUMP | Status pad pump 0=OFF 1=ON |  | I134 The status of the pad pump.
REG_FAN.AANTAL_FAN_AKT | 20A | F&P CONTR | Number of active fan stages |  | I130 The number of active fan stages by the calculated fan capacity and forced by for example curtains, rain, storm or frost. I133 The number of connected fan stages in the ON and FORCED ON statuses. M100 The measured number of active fan stages. M106 The measured number of active fan stages. M130 The number of active fan stages by the calculated fan capacity and forced by for example curtains, rain, storm or frost.
REG_FAN.TOEST_FANR | 20D | F&P CONTR | Status fan control 0=NOT ACTIVE 1=ACTIVE 2=SWITCH ON 3=SWITCH OFF 4=ROTATE |  | I133
REG_PEF.BER_VENT_CAP | 216 | F&P CONTR | Calculated fan capacity | % | I130 The degree to which F&P cooling is desirable. The calculated fan capacity determines the number of fan stages and the switching moment of the pad pump. M130 The degree to which F&P cooling is desirable. The calculated fan capacity determines the number of fan stages and the switching moment of the pad pump.
REG_PEF.GEW_FAN_AKT | 218 | F&P CONTR | Calc number of fan stages |  | I130 The calculated maximum number of fan stages that is allowed to be active. M130 The calculated maximum number of fan stages that is allowed to be active.
REG_PEF.PEF_AKTIEF | 221 | F&P CONTR | fan and pad cooling active 0=NO 1=YES |  | I130 Indication of whether the F&P cooling is active. M130 Indication of whether the F&P cooling is active.
REG_PEF.REFERENTIE | 225 | F&P CONTR | fan and pad cooling temperature | °C | M106
REG_PEF.START_PEF | 226 | F&P CONTR | fan and Pad cooling temperature | °C | I130 The calculated (greenhouse) temperature limit above which the F&P cooling becomes active. M106 M130 The calculated (greenhouse) temperature limit above which the F&P cooling becomes active.
VntsPBand.CalcPBand100p | 6348 | VENT.CONTR | calculated P band | °C | M125.1 The calculated P band, depending on the set (minimum and maximum) P band, the weather influence on the P band and the increase & decrease time over which the vents are moved from 0% to 100%.
KASL_REF.ATR_GEM_KAS_TEMP | 37D | VENT.CONTR | ventilation temperature | °C | I100 The measured ventilation temperature (greenhouse or plant temperature). M100 The measured ventilation temperature (greenhouse or plant temperature).
VENTAFST.STW_RAAM | 4B0 | VENT.CONTR | Calc ventilation temperature | °C | I120 The calculated ventilation temperature after influencing. I121 M100 The calculated ventilation temperature. M100.1 The calculated ventilation temperature. M106
VntsControl.ActAirExchange | 3A7 | VENT.CONTR | Calc air exchange | m³/(hr.m²) | M120 The calculated air exchange for the ventilation control.
VntsControl.MeasCtrlTemp | 4B4 | VENT.CONTR | ventilation temperature | °C | M106
VntsLeeSide.CalcMaxVentLee | 60BA | VENT.CONTR | Calculated max vent lee | % | M125 The calculated maximum vent position for the lee side after possible limitations.
VntsLeeSide.CalcMinVentLee | 417 | VENT.CONTR | Calculated min vent lee | % | M125 The calculated minimum vent position on the lee side.
VntsLeeSide.CalcVentLeePos | 3D4 | VENT.CONTR | Calculated vent lee | % | M125 The calculated vent position on the lee side.
VntsLeeSide.CalcVtTempLee | 60BD | VENT.CONTR | Calc ventilation temperature lee | °C | M120 As soon as the measured temperature rises above the ventilation temperature calculated here for the lee side, then on the lee side the vents will start to be controlled open.
VntsLeeSide.CodeLimitMnLee | 60BF | VENT.CONTR | Limitation min vent lee 0=NONE 1=MIN 2=CROP TREATM. 3=CURTAIN 4=ON/OFF HEAT 5=RAIN 6=FROST 7=STORM 8=MAX 9=F&P 10=W ROBOT 11=SUN 12=HUMIDITY 13=LEE SIDE 14=WIND 15=AIR EXCHANGE 16=OUTLET 17=RELEASE 18=SHOWER PROT.P1 19=SHOWER PROT.P2 20=EXTRA INFLUENCE 21=DEV. TEMP 22=CROP ACT. 23=INSTALLATION 24=INCREASE 25=AIR CIRCULATION |  | M125 Indication of the limitation of the minimum vent position on the lee side. See Beperking_raamstand_Connext.
VntsLeeSide.CodeLimitMxLee | 60C0 | VENT.CONTR | Limitation max vent lee 0=NONE 1=MIN 2=CROP TREATM. 3=CURTAIN 4=ON/OFF HEAT 5=RAIN 6=FROST 7=STORM 8=MAX 9=F&P 10=W ROBOT 11=SUN 12=HUMIDITY 13=LEE SIDE 14=WIND 15=AIR EXCHANGE 16=OUTLET 17=RELEASE 18=SHOWER PROT.P1 19=SHOWER PROT.P2 20=EXTRA INFLUENCE 21=DEV. TEMP 22=CROP ACT. 23=INSTALLATION 24=INCREASE 25=AIR CIRCULATION |  | M125 Indication of the limitation of the maximum vent position on the lee side. See Beperking_raamstand_Connext.
VntsLeeSide.MeasVentLeePos | 3DE | VENT.CONTR | Measured vent lee | % | M125 The measured vent position on the lee side.
VntsWindSide.CalcMaxVentWind | 60DA | VENT.CONTR | Calculated max vent wind | % | M125
VntsWindSide.CalcMinVentWind | 418 | VENT.CONTR | Calculated min vent wind | % | M125
VntsWindSide.CalcVentWindPos | 3D6 | VENT.CONTR | Calculated vent wind | % | M125
VntsWindSide.CalcVtTempWind | 3EA | VENT.CONTR | Calc ventilation temperature wind | °C | M120 As soon as the measured temperature rises above the ventilation temperature calculated here for the wind side, then on the wind side the vents will start to be controlled open.
VntsWindSide.CodeLimitMnWind | 3F1 | VENT.CONTR | Limitation min vent wind 0=NONE 1=MIN 2=CROP TREATM. 3=CURTAIN 4=ON/OFF HEAT 5=RAIN 6=FROST 7=STORM 8=MAX 9=F&P 10=W ROBOT 11=SUN 12=HUMIDITY 13=LEE SIDE 14=WIND 15=AIR EXCHANGE 16=OUTLET 17=RELEASE 18=SHOWER PROT.P1 19=SHOWER PROT.P2 20=EXTRA INFLUENCE 21=DEV. TEMP 22=CROP ACT. 23=INSTALLATION 24=INCREASE 25=AIR CIRCULATION |  | M125
VntsWindSide.CodeLimitMxWind | 3EF | VENT.CONTR | Limitation max vent wind 0=NONE 1=MIN 2=CROP TREATM. 3=CURTAIN 4=ON/OFF HEAT 5=RAIN 6=FROST 7=STORM 8=MAX 9=F&P 10=W ROBOT 11=SUN 12=HUMIDITY 13=LEE SIDE 14=WIND 15=AIR EXCHANGE 16=OUTLET 17=RELEASE 18=SHOWER PROT.P1 19=SHOWER PROT.P2 20=EXTRA INFLUENCE 21=DEV. TEMP 22=CROP ACT. 23=INSTALLATION 24=INCREASE 25=AIR CIRCULATION |  | M125
VntsWindSide.MaxRFallPh1Wind | 413 | VENT.CONTR | Max vent wind rainfall radar phase 1 | % | I125.1 Limitation of the vent position on the wind side if the rainfall radar is forecasting a precipitation intensity that is greater than the intensity specified for phase 1.
VntsWindSide.MeasVentWindPos | 60E3 | VENT.CONTR | Measured vent wind | % | M125
ALG_POMP_.POMP_DRAAIT | 56F | WATER TEMP | Pump active 0=NO 1=YES |  | M115.2 Indication of whether the circulation pump has been activated.
RVW_BUIS.MAX_BUIS | 632 | WATER TEMP | calculated maximum water temperature | °C | I115 Calculated pipe temperatures. I116 M115 The calculated maximum water temperature after the influence(s).
RVW_BUIS.MIN_BUIS | 633 | WATER TEMP | calculated minimum water temperature | °C | I115 Calculated pipe temperatures. I116 M115 The calculated minimum water temperature after the influence(s).
VERWNET.BER_BUIS_T | 651 | WATER TEMP | calculated water temperature | °C | M100.1 The calculated water temperature. M106 M115 The calculated water temperature.
VERWNET.GEM_BUIS_T | 652 | WATER TEMP | water temperature | °C | M100 The measured pipe temperature M106 M115 The measured pipe temperature
VN_RETOUR.GEM_RET_TEMP | 658 | WATER TEMP | water temperature return | °C | M100 The measured return temperature of the pipe. M115 The measured return water temperature.
VNET_STREEF.GESEL_MAX_BUIST | 674 | WATER TEMP | Set max water temperature | °C | M115 The set maximum water temperature of the period that is currently activated.
VNET_STREEF.GESEL_MIN_BUIST | 675 | WATER TEMP | Set min water temperature | °C | M115 The set minimum water temperature of the period that is currently activated.
KASL_REF.ATR_GEM_KAS_TEMP | 6A3 | HEAT CONTR | heating temperature | °C | I100 The measured heating temperature (greenhouse or plant temperature). M100 The measured heating temperature (greenhouse or plant temperature).
MODVERW_.GER_AUT_VERM | 6CB | HEAT CONTR | Act capacity aut heat system | kW | M112 The actual capacity by the autonomous heating systems.
VERWCTL.GER_EXT_VERM | 6E3 | HEAT CONTR | Total external capacity | kW | M112 Total sum of the external capacities which influence the capacity demand of the heating control provided by HID lighting and hot air heaters.
VERWCTL.GEW_KASTEMP | 6E5 | HEAT CONTR | desired heating temperature | °C | M100 The calculated heating temperature. M100.1 The calculated heating temperature. M106 The calculated heating temperature is the same for the heating controls. M110 The calculated heating temperature which takes into account influences, maximum increase and maximum decrease of I110.1 Verwarming/Invloeden and temperature balance control. M112 The calculated heating temperature which takes into account influences, maximum increase and maximum decrease of I110.1 Verwarming/Invloeden and temperature balance control.
VERWCTL.GEW_VERM_MODVW | 6E7 | HEAT CONTR | Des capacity heat total | kW | M112 The desired capacity for keeping the greenhouse at the correct temperature or getting it there.
VERWCTL.REFERENTIE | 6F6 | HEAT CONTR | measured heating temperature | °C | M106 The calculated heating temperature is the same for the heating controls.
DKMAN.GEW_DKFUNC | 8D2 | CURT CONTR | Desired curtain function 0=NONE 1=HUMIDITY 2=SHADING 3=ENERGY 4=BLACK OUT 5=SLAVE 6=SIDE |  | M160 Indication of the desired (new) curtain function.
EnergCurGen_Calc.CurTotalCond | 5E48 | CURT CONTR | Calculated status curtain 0=CLOSE 1=OPEN |  | M162 Indicates the desired curtain position, taking into account all the set conditions.
EnergCurGen_Calc.LimitEnergCurStr | 5E5D | CURT CONTR | Limitation energy curtain strategy 0=NONE 1=PER. END TIME 2=FORCED OPEN 3=FORCED CLOSE 4=AUTO OPEN 5=AUTO CLOSE 6=SHOWER PROT. |  | M162
ENSTR_STEPS.DkPrBovenDkTlu | 5EF3 | CURT CONTR | Meas temperature above curtain | °C | I162.1 M162
GapControl.CalcedGapSize | 928 | CURT CONTR | gap size actual | % | I165 M160 The calculated gap size is the largest of the calculated temperature gaps and the calculated humidity gap.
GapControl.DeltaHumAvg | 931 | CURT CONTR | measured difference humidity | g/m³ | I165
GapControl.DeltaTempAvg | 932 | CURT CONTR | measured difference temperature | °C | I165
RVSTW_SAVE.GEW_DKST | 9B3 | CURT CONTR | Calculated humidity curtain position | % | I164
SCSTW.ScDkStandDemp | 9D3 | CURT CONTR | Calculated shading curtain position | % | I163
SDK_StralRef.StralRefVsGem | 9DB | CURT CONTR | Used radiation | W/m² | I160.4 The radiation that is used to control the shading curtain in the compartment. I160.4 The radiation that is used to control the autonomous shading curtain. I163
VDSTW.GEW_DKST | 9DF | CURT CONTR | Calculated black out curtain position | % | I161
VERD_StralRef.StralRefVsGem | 9F1 | CURT CONTR | applied radiation black out curtain | W/m² | I160.4 The radiation that is used to control the black out curtain in the compartment. I160.4 The radiation that is used to control the autonomous black out curtain.
VerdDoekPer.VoorwaardeGeldig | A18 | CURT CONTR | Condition valid 0=NO 1=YES |  | I161
vlg_doek.BER_DOEKST | A1B | CURT CONTR | Calculated side-slave curtain position | % | I166
vlg_doek.MAX_DOEKST | A1E | CURT CONTR | Max curtain position | % | I166 Maximum curtain position when the curtain is controlled shut from the side-slave curtain function.
DKST_VB.BEGR_CODE | A4F | CURTAIN | Curtain position limitation 0=NONE 1=VENTS 2=ELECTR 3=RELEASE 4=CLOCK 5=FIXED 6=INSTALLATION 7=LIGHTING 8=CROP TREATM. 9=VENTIL 10=GAP 12=STORM 13=EXTERNAL MAX 14=EXTERNAL MIN 15=SHOWER PROT.P1 16=SHOWER PROT.P2 17=LIGHT EMISSION |  | I168 Indication of the current curtain position limitation. M160 Indication of the current curtain position limitation, see I168 Doek sturing.
DKST_VB.BER_DKST | 67AA | CURTAIN | Calculated curtain position | % | M160 The calculated curtain position from the Actual curtain function .
DKST_VB.DK_FUNC | A56 | CURTAIN | Actual curtain function 0=NONE 1=HUMIDITY 2=SHADING 3=ENERGY 4=BLACK OUT 5=SLAVE 6=SIDE |  | I168 The active curtain function that determines the curtain position if necessary in combination with a gap control. M160 The curtain function that is valid at this moment.
DKST_VB.DoekStandGer | A5C | CURTAIN | Measured curtain position | % | M100 The measured curtain position in the compartment. M160 The measured curtain position at curtain position measurement and the current curtain position calculated from the run time.
DKST_VB.GEW_DKST | A62 | CURTAIN | Desired curtain position | % | M160
PARMe.PARGemMed | BBB | PAR SENSOR | PAR | umol/s/m² | M4 M105 The measured PAR in the compartment. If there are several PAR measurements in the compartment, select which measurement is displayed here in I100.3 Installations/Radiation and compartment.
afd_groeilicht.Ger_niveau | CDA | CMP | Number of active growing light steps |  | M106 Number of growing light steps switched on (undelayed)
AFD_SOM.BER_AFD_STRAL | CE1 | CMP | calculated radiation greenhouse | W/m² | M100 The calculated radiation in the compartment. This value is calculated based on the measured radiation outside, the height of the sun, the system and its usage. No account is taken of conditions such as whitewashing or pollution of the greenhouse roof, condensation on the greenhouse roof or aging of the (growing light) installation.
AFD_SOM.BER_ASS_STRAL | CE3 | CMP | calculated radiation growing light | W/m² | M100 The calculated radiation emitted by the growing light.
AfdRegElekSm.ElecTdCompTot | CFA | CMP | Electr.total | kWh | M107 Cumulative electricity consumption from the set time in the 24-hour period of all growing light systems and air treatment systems of this compartment.
AfdRegElekSm.ElecTdCompTotM2 | CF9 | CMP | Electr per m² | kWh/m² | M107 Cumulative electricity consumption from the set time in the 24-hour period of all growing light systems and air treatment systems per m² of this compartment.
AfdRegElekSm.ElecYdCompTot | CF8 | CMP | Electr.total | kWh | M107
AfdRegElekSm.ElecYdCompTotM2 | CF7 | CMP | Electr per m² | kWh/m² | M107
AfdRegGasSm.GasSmTd_m2 | CFD | CMP | Gas per m² | m³/m² | M107 The gas consumption of today per m² of the compartment.
AfdRegGasSm.GasSmTd_tot | CFE | CMP | Gas total | m³ | M107 The total gas consumption of today of the compartment.
AfdRegGasSm.GasSmYd_m2 | CFB | CMP | Gas per m² | m³/m² | M107
AfdRegGasSm.GasSmYd_tot | CFC | CMP | Gas total | m³ | M107
DryPhase.CurrentDryPhase | D22 | CMP | Active dry phase |  | M106 Irrigation has taken place and the stated drying phase is active.
DryPhase.IrrigationActive | D23 | CMP | Irrigation active 0=NO 1=YES |  | M106 The irrigation is active.
GEM_GEWASTEMP.GEM_GEWAS_RV | D29 | CMP | relative humidity | % | M100 The calculated relative air humidity at the measured plant temperature.
GEM_GEWASTEMP.GEM_GEWAS_TEMP | D2A | CMP | Measured plant temperature | °C | M100
GEM_GEWASTEMP.GEM_GEWAS_VD | D2B | CMP | humidity deficit | g/m³ | M100 The calculated humidity deficit for the measured plant temperature.
GEM_GEWASTEMP.GEM_GEWAS_VPD | D2C | CMP | VPD | kPa | M100 The calculated vapour pressure deficit for the measured plant temperature. The vapour pressure deficit is the difference between the vapour pressure in the crop's stomata and the vapour pressure in the greenhouse air.
INVL_FAC_VERW.GESEL_VWTEMP | D40 | CMP | Corrected heating temperature | °C | M110 The heating temperature, corrected if applicable by the 24h temperature control. This temperature may also be a correction setting.
INVL_FAC_VERW.STW_VERW | D4E | CMP | Calc heating temperature | °C | I110 Calculated heating temperature after influence(s). I111 M110 The calculated heating temperature which takes into account influences, maximum increase and maximum decrease in I110.1 Heating/Influences.
KASL_REF.ATR_GEM_KAS_AV | D58 | CMP | absolute humidity | g/m³ | M100 The measured absolute air humidity.
KASL_REF.ATR_GEM_KAS_CO2 | D59 | CMP | CO₂ | ppm | M100
KASL_REF.ATR_GEM_KAS_RV | D5A | CMP | relative humidity | % | M100 The measured relative air humidity.
KASL_REF.ATR_GEM_KAS_TEMP | D5B | CMP | greenhouse temperature | °C | M100 The measured greenhouse air temperature.
KASL_REF.ATR_GEM_KAS_VD | D5C | CMP | humidity deficit | g/m³ | M100 The measured humidity deficit.
LuchtConditie.ActieveFase | D88 | CMP | active phase crop treatment 0=OFF 1=PHASE 1 2=PHASE 2 3=PHASE 3 4=PHASE 4 5=PHASE 5 6=PHASE 6 |  | M106 The active phase of the crop treatment strategy.
PAR_Ref.PARRefVsGem | D8E | CMP | Measured | umol/s/m² | I100 The measured PAR level in the compartment. M100 The measured PAR in the compartment. If there are several PAR measurements in the compartment, select which measurement is displayed here in I100.3 Installations/Radiation and compartment.
Temp24hour.Actual24hTemp | E19 | CMP | Actual 24 hours temperature current 24 hours | °C | I104
Temp24hour.ActualCorrPerc | E1A | CMP | calculated correction | % | I104
Temp24hour.ActualRTRvalPAR | 7D86 | CMP | Actual RTR per 10 mol/m² current 24 hours | °C | I104
Temp24hour.ActualRTRvalRad | 7D87 | CMP | Actual RTR per 1000 J/cm² current 24 hours | °C | I104
Temp24hour.DeviationState | E23 | CMP | calculated control action 0=NONE 1=DECREASE 2=INCREASE |  | I104
Temp24hour.Exp24hTActual | E25 | CMP | Expected 24 hours temperature until now | °C | I104
Temp24hour.Final24hTemp | E27 | CMP | Desired 24 hours temperature current 24 hours | °C | I104 I104 I104
Temp24hour.PrevActual24hT | E30 | CMP | Actual 24 hours temperature previous 24 hours | °C | I104
Temp24hour.PrevBase24hTemp | 7DB5 | CMP | Set base temperature previous 24 hours | °C |
Temp24hour.PrevFinal24hT | E31 | CMP | Desired 24 hours temperature previous 24 hours | °C | I104
Temp24hour.PrevPARSmOutside | 7DB7 | CMP | Actual RTR PAR sum outside previous 24 hours | mol/m² |
Temp24hour.PrevPARSumInside | 7DB8 | CMP | Actual RTR PAR sum inside previous 24 hours | mol/m² |
Temp24hour.PrevRadSmOutside | 7DB9 | CMP | Actual RTR radiation sum outside previous 24 hours | J/cm² |
Temp24hour.PrevRadSumInside | 7DBA | CMP | Actual RTR radiation sum inside previous 24 hours | J/cm² |
Temp24hour.PrevRTRvaluePAR | 7D8A | CMP | Actual RTR per 10 mol/m² previous 24 hours | °C | I104
Temp24hour.PrevRTRvalueRad | 7D8B | CMP | Actual RTR per 1000 J/cm² previous 24 hours | °C | I104
Temp24hour.PrevSetRTRperKJ | 7DBB | CMP | Set RTR per 1000 J/cm² previous 24 hours | °C |
Temp24hour.PrevSetRTRperMol | 7DBC | CMP | Set RTR per 10 mol/m² previous 24 hours | °C |
TempStrategy.RecipeHeatTemp | E40 | CMP | Set heating temperature | °C | M110 The set heating temperature of the period that is currently activated.
TempStrategy.RecipeVentTemp | E3F | CMP | Set ventilation temperature | °C | M120 The set ventilation temperature of the period that is currently activated.
TrAfdPARSomRef.PARRefSomBer | E44 | CMP | PAR sum | mol/m² | M100 The measured PAR sum in the compartment counted from the moment of sunrise (M4 Overzicht/Metingen).
UI_KOEL.BER_KOEL_TEMP | E49 | CMP | cooling temperature calculated | °C | I220 Calculated temperature of the cold store, greenhouse or greenhouse soil. M106
UI_KOEL.BER_VRIJG | E4A | CMP | Release cooling 0=NO 1=YES |  | I220 Indication of whether the cooling has been released.
VENTSTREEF.GES_STW_RAAM | E73 | CMP | Corrected ventilation temperature | °C | M120 The ventilation temperature, corrected if applicable by the 24h temperature control. This temperature may also be a correction setting.
ZonHoogte.StrDoorlaatAlg | E96 | CMP | translucency greenhouse roof | % | I101 The translucency used from the greenhouse roof. The translucency is used for several controls, such as the light control, the heating control, the ventilation control, the transpiration sum start in the irrigation and for the calculation of the top temperature of the crop.
Afname_Trafo.ActualCapacity | 6A30 | OFF-TAKE TRA | Act. electrical capacity | kW | M200 The sum of the total maximum electrical capacity of all the growing light systems and other electrical consumers connected to this off-take transformer.
Afname_Trafo.CalcLimitation | 6A31 | OFF-TAKE TRA | Limitation 0=NONE 1=BLOCK 2=DEMAND MAX 3=INSTAL MAX |  | M200 The limitation of the desired electrical capacity of this off-take transformer.
Afname_Trafo.DesiredCapacity | 6A32 | OFF-TAKE TRA | Des electrical capacity | kW | M200 The sum of the total desired capacity that must be supplied to all the connected consumers.
Afname_Trafo.Meas_Sper | 6A37 | OFF-TAKE TRA | Used value 0=NO 1=YES |  | M200
DKMAN.GEW_DKFUNC | 1094 | CURT CONTR | Desired curtain function 0=NONE 1=HUMIDITY 2=SHADING 3=ENERGY 4=BLACK OUT 5=SLAVE 6=SIDE |  | M160 Indication of the desired (new) curtain function.
EnergCurGen_Calc.CurTotalCond | 5E59 | CURT CONTR | Calculated status curtain 0=CLOSE 1=OPEN |  | M162 Indicates the desired curtain position, taking into account all the set conditions.
EnergCurGen_Calc.LimitEnergCurStr | 5E72 | CURT CONTR | Limitation energy curtain strategy 0=NONE 1=PER. END TIME 2=FORCED OPEN 3=FORCED CLOSE 4=AUTO OPEN 5=AUTO CLOSE 6=SHOWER PROT. |  | M162
ENSTR_STEPS.DkPrBovenDkTlu | 5F16 | CURT CONTR | Meas temperature above curtain | °C | I162.1 M162
GapControl.CalcedGapSize | 10EA | CURT CONTR | gap size actual | % | I165 M160 The calculated gap size is the largest of the calculated temperature gaps and the calculated humidity gap.
GapControl.DeltaHumAvg | 10F3 | CURT CONTR | measured difference humidity | g/m³ | I165
GapControl.DeltaTempAvg | 10F4 | CURT CONTR | measured difference temperature | °C | I165
RVSTW_SAVE.GEW_DKST | 1175 | CURT CONTR | Calculated humidity curtain position | % | I164
SCSTW.ScDkStandDemp | 1195 | CURT CONTR | Calculated shading curtain position | % | I163
SDK_StralRef.StralRefVsGem | 119D | CURT CONTR | Used radiation | W/m² | I160.4 The radiation that is used to control the shading curtain in the compartment. I160.4 The radiation that is used to control the autonomous shading curtain. I163
VDSTW.GEW_DKST | 11A1 | CURT CONTR | Calculated black out curtain position | % | I161
VERD_StralRef.StralRefVsGem | 11B3 | CURT CONTR | applied radiation black out curtain | W/m² | I160.4 The radiation that is used to control the black out curtain in the compartment. I160.4 The radiation that is used to control the autonomous black out curtain.
VerdDoekPer.VoorwaardeGeldig | 11DA | CURT CONTR | Condition valid 0=NO 1=YES |  | I161
vlg_doek.BER_DOEKST | 11DD | CURT CONTR | Calculated side-slave curtain position | % | I166
vlg_doek.MAX_DOEKST | 11E0 | CURT CONTR | Max curtain position | % | I166 Maximum curtain position when the curtain is controlled shut from the side-slave curtain function.
DKST_VB.BEGR_CODE | 1211 | CURTAIN | Curtain position limitation 0=NONE 1=VENTS 2=ELECTR 3=RELEASE 4=CLOCK 5=FIXED 6=INSTALLATION 7=LIGHTING 8=CROP TREATM. 9=VENTIL 10=GAP 12=STORM 13=EXTERNAL MAX 14=EXTERNAL MIN 15=SHOWER PROT.P1 16=SHOWER PROT.P2 17=LIGHT EMISSION |  | I168 Indication of the current curtain position limitation. M160 Indication of the current curtain position limitation, see I168 Doek sturing.
DKST_VB.BER_DKST | 67AB | CURTAIN | Calculated curtain position | % | M160 The calculated curtain position from the Actual curtain function .
DKST_VB.DK_FUNC | 1218 | CURTAIN | Actual curtain function 0=NONE 1=HUMIDITY 2=SHADING 3=ENERGY 4=BLACK OUT 5=SLAVE 6=SIDE |  | I168 The active curtain function that determines the curtain position if necessary in combination with a gap control. M160 The curtain function that is valid at this moment.
DKST_VB.DoekStandGer | 121E | CURTAIN | Measured curtain position | % | M100 The measured curtain position in the compartment. M160 The measured curtain position at curtain position measurement and the current curtain position calculated from the run time.
DKST_VB.GEW_DKST | 1224 | CURTAIN | Desired curtain position | % | M160
REG_PEF.BER_VENT_CAP | 14EB | AUT F&P | Calculated fan capacity | % |
REG_PEF.REFERENTIE | 14FA | AUT F&P |  | °C | M106
REG_PEF.START_PEF | 14FB | AUT F&P | Temperature F&P cooling active | °C |
KASL_REF.ATR_GEM_KAS_TEMP | 1669 | AUT VENT | ventilation temperature | °C |
TempStrategy.RecipeVentTemp | 1781 | AUT VENT | Set ventilation temperature | °C | M120 The set ventilation temperature of the period that is currently activated.
VENTAFST.STW_RAAM | 17A6 | AUT VENT | Calc ventilation temperature | °C |
VENTSTREEF.GES_STW_RAAM | 17B8 | AUT VENT | Corrected ventilation temperature | °C | M120 The ventilation temperature, corrected if applicable by the 24h temperature control. This temperature may also be a correction setting.
VntsControl.MeasCtrlTemp | 17AA | AUT VENT |  | °C | M106
VntsLeeSide.CalcMaxVentLee | 60BB | AUT VENT | Calculated max vent lee | % | M125 The calculated maximum vent position for the lee side after possible limitations.
VntsLeeSide.CalcMinVentLee | 1703 | AUT VENT | Calculated min vent lee | % | M125 The calculated minimum vent position on the lee side.
VntsLeeSide.CalcVentLeePos | 16C0 | AUT VENT | Calculated vent lee | % | M125 The calculated vent position on the lee side.
VntsLeeSide.CalcVtTempLee | 60BC | AUT VENT | Calc ventilation temperature lee | °C | M120 As soon as the measured temperature rises above the ventilation temperature calculated here for the lee side, then on the lee side the vents will start to be controlled open.
VntsLeeSide.MeasVentLeePos | 16CA | AUT VENT | Measured vent lee | % | M125 The measured vent position on the lee side.
VntsWindSide.CalcMaxVentWind | 60DB | AUT VENT | Calculated max vent wind | % | M125
VntsWindSide.CalcMinVentWind | 1704 | AUT VENT | Calculated min vent wind | % | M125
VntsWindSide.CalcVentWindPos | 16C2 | AUT VENT | Calculated vent wind | % | M125
VntsWindSide.CalcVtTempWind | 16D6 | AUT VENT | Calc ventilation temperature wind | °C | M120 As soon as the measured temperature rises above the ventilation temperature calculated here for the wind side, then on the wind side the vents will start to be controlled open.
VntsWindSide.MeasVentWindPos | 60E2 | AUT VENT | Measured vent wind | % | M125
ALG_POMP_.POMP_DRAAIT | 1A14 | AUT HEAT | Pump active 0=NO 1=YES |  |
INVL_FAC_VERW.GESEL_VWTEMP | 1A5B | AUT HEAT | Corrected heating temperature | °C | M110 The heating temperature, corrected if applicable by the 24h temperature control. This temperature may also be a correction setting.
INVL_FAC_VERW.STW_VERW | 1A69 | AUT HEAT | Calc heating temperature | °C |
KASL_REF.ATR_GEM_KAS_TEMP | 1A72 | AUT HEAT | heating temperature | °C |
RVW_BUIS.MAX_BUIS | 1B3A | AUT HEAT | calculated maximum water temperature | °C |
RVW_BUIS.MIN_BUIS | 1B3B | AUT HEAT | calculated minimum water temperature | °C |
TempStrategy.RecipeHeatTemp | 1B63 | AUT HEAT | Set heating temperature | °C | M110 The set heating temperature of the period that is currently activated.
VERWCTL.GER_EXT_VERM | 1B8C | AUT HEAT | Total external capacity | kW | M112 Total sum of the external capacities which influence the capacity demand of the heating control provided by HID lighting and hot air heaters.
VERWCTL.GER_VERM | 1B8D | AUT HEAT | Act capacity heat system | kW | M112 The actual capacity by the heating system.
VERWCTL.GEW_KASTEMP | 1B8E | AUT HEAT | desired heating temperature | °C |
VERWCTL.GEW_VERM_MODVW | 1B90 | AUT HEAT | Des capacity heat total | kW | M112 The desired capacity for keeping the greenhouse at the correct temperature or getting it there.
VERWCTL.REFERENTIE | 1B9F | AUT HEAT |  | °C | M106 The calculated heating temperature is the same for the heating controls.
VERWNET.BER_BUIS_T | 1BAC | AUT HEAT | calculated water temperature | °C |
VERWNET.GEM_BUIS_T | 1BAE | AUT HEAT | Meas water temperature | °C |
VNET_STREEF.GESEL_MAX_BUIST | 1BD1 | AUT HEAT | Set max water temperature | °C | M115 The set maximum water temperature of the period that is currently activated.
VNET_STREEF.GESEL_MIN_BUIST | 1BD2 | AUT HEAT | Set min water temperature | °C | M115 The set minimum water temperature of the period that is currently activated.
KASLBOX.GEM_CO2 | 1D72 | AUT REF | CO₂ | ppm |
KASLBOX.GEM_KAS_RV | 1D73 | AUT REF | relative humidity | % |
KASLBOX.GEM_KAS_VD | 1D74 | AUT REF | humidity deficit | g/m³ |
KASLBOX.GEM_KASNBOL | 1D75 | AUT REF | WBT | °C |
KASLBOX.GEM_KASTEMP | 1D76 | AUT REF | temperature | °C |
PAR_Ref.PARRefVsGem | 21AD | GR. PROGR | applied PAR | umol/s/m² | I205 I205.4 The used PAR for the growing light program.
Stral_Ref.StralRefVsGem | 21B2 | GR. PROGR | Used radiation | W/m² | I205 I205.4 The used radiation for the growing light program.
STW_ASSB.CdBelAan | 21B7 | GR. PROGR | Switch on desire 0=NONE 1=LIGHTING 2=EXTERNAL |  | I205 Indication of the desire to switch on the growing light.
STW_ASSB.CdBep | 21B8 | GR. PROGR | Limitation 0=NONE 1=MEAS RAD. SUM 2=MEAS PAR SUM 3=EXP RAD. SUM 4=EXP PAR SUM 5=LONG DAY 6=EXTERN OFF 7=ADJUST LIMIT 8=REL.OUTSIDE TEMP 9=EXTERN ON |  | I205
STW_ASSB.GER_STRAL_SOM | 21BB | GR. PROGR | radiation sum today | J/cm² | I205
STW_ASSB_PAR.AbPrPARGerSomVd | 21C3 | GR. PROGR | PAR sum today | mol/m² | I205
VERW_PAR_SOM.HuidigEtmaal | 21C7 | GR. PROGR | expected PAR sum today | mol/m² | I205
KDAS_STU.BER_BEPERKING | 21D0 | STRING | Limitation 0=NONE 1=RADSUM 2=MIN T ON 3=MIN T OFF 4=WAIT REL 5=END TIME 6=WAIT HEAT ON 7=WAIT HEAT OFF 8=CROP TREATM. 9=WAIT CURTAIN 10=REL.OUTSIDE TEMP 11=FIXED POS, OFF 12=FIXED POS, ON 13=EXTERN OFF 14=EXTERN ON 15=DEALER DRIVE 16=INSTALLATION 17=PERIOD SWITCH OFF 18=LOCAL BLOCK 19=ALWAYS FORCED OFF |  | I206 The limitation for the string of the growing light system. M205 See I206 Groeilicht systeem/Realisatie.
KDAS_STU.TOEST_UITG | 21DC | STRING | Act status string 0=OFF 1=ON |  | I206 Actual status of the string. M205 The actual status of string X of the growing light system.
AB_SYS.GER_AB_TOEST | 21E8 | SW. LIGHT | Actual status 0=OFF 1=MIN T OFF 2=WAIT REL 3=ON 4=MIN T ON 5=WAIT ON 6=WAIT OFF |  | I206
AB_SYS.gew_ab_toest | 21EA | SW. LIGHT | 0=OFF 1=ON |  |
KRAANGRP.DOORLOOP | 2234 | VALVE GRP | Number of times phase active |  | I401 Indication of the number of times (see 17 Number of times phase ) that the phase has been run. This can be used to follow the progress of the irrigation.
KRAANGRP.HWATER_STRALSOM | 223E | VALVE GRP | highest quantity water per radiation sum | ml/MJ | M100 The highest water dosage of the valve group. M430 The highest water dosage of the valve group. Deviations are reported, see Meldingen en alarmen.
KRAANGRP.LWATER_STRALSOM | 2244 | VALVE GRP | lowest quantity water per radiation sum | ml/MJ | M100 The lowest water dosage of the valve group. The Water per rad.sum is the quantity of water per radiation sum, determined over the last 3 irrigation cycles. M430 The lowest water dosage of the valve group. The quantity of water per radiation sum, determined over the last 3 irrigation cycles. Deviations are reported, see Meldingen en alarmen.
KRAANGRP.TOESTAND | 2253 | VALVE GRP | Status valve group 0=REST 1=WAITING 2=PHASE 1 3=PHASE 2 4=PHASE 3 5=PHASE 4 6=PHASE 5 7=WAIT 8=EXT WAIT 9=PHASE WAIT 10=ABORT 11=ERROR 1 12=ERROR 2 13=ERROR 3 14=ERROR 4 15=ERROR 5 |  | I401 Status indication of the valve group. I402 Status indication of the valve group. M100 See Status in I402 Handstart/Kraangroep & start. M430 See Status in I402 Handstart/Kraangroep & start.
NET_ELB.BEPERKING | 2262 | ELECTR.NETW | Limitation 0=NONE 1=BLOCK |  | M200 The limitation of the electricity network.
NET_ELB.BRON_PRODUCEERT | 2263 | ELECTR.NETW | Electricity production active 0=NO 1=YES |  | M200 Indication whether the electricity production by the network is active.
NET_ELB.GemVeExpMom | 2267 | ELECTR.NETW | Measured electrical export | kW | M200 Measured quantity of electricity that is supplied to the electricity network.
NET_ELB.GemVeImpMom | 2268 | ELECTR.NETW | Measured electrical import | kW | M200 Measured quantity of electricity that the electricity network supplies.
NET_ELB.GER_CAP_BRON | 2269 | ELECTR.NETW | Max electrical capacity | kW | M200 The maximum electrical capacity to be supplied by the electricity network.
NET_ELB.GEW_VERM_BRON | 226A | ELECTR.NETW | Des electrical capacity | kW | M200 The electrical capacity demanded from the electricity network.
MENGER.BEPERKING | 2307 | MIXER | Limitation 0=NONE 1=CHANNEL 2=NO TANK 3=CONFIGURATION 4=STEP 5=POWER FAILURE 6=EXT ERROR 7=PUMP ERROR 8=FLOW TOO LOW 9=FLOW TOO HIGH 10=LEAKAGE ! 11=MONITOR WATER VALVE 12=OPEN WATER VALVE 13=MONITOR FERTILIZER 14=OPEN FERTILIZER 15=TANK 0 LITER 20=SELECT TANK 21=FRESH WATER 30=FLOW DEFECTIVE 31=ALARM SELECT TANK 32=ALARM PUMP TANK 33=LEVEL TOO HIGH TANK 41=ALARM SEL INT TANK 42=AL PUMP INTERM TANK 43=AL DRAIN INTER TANK 44=AL RINSE INTER TANK 45=LEVEL TOO HIGH ITNK 46=INT TANK NOT EMPTY 47=ERROR INTERM TANK 100=I/O WATER VALVE 101=I/O PUMP 102=I/O SELECT TANK 103=I/O SEL INTERM TANK 104=I/O PUMP TANK 105=I/O MIX CHANNEL 106=I/O FLOW 107=I/O DRAIN INT.TANK 108=I/O RINSE INT. TANK 110=START RINSE 111=MINIMUM RINSE 112=MAXIMUM RINSE 113=END RINSE |  | I428 I428.1 See I428 Meststof instellingen
MENGER.BUSY_STAP | 2309 | MIXER | Step |  | I428.1 The current step in the mixing process, you can find an overview of all steps in line 2.
MENGER.BUSY_TOESTAND | 230A | MIXER | Status step 0=--- 1=STOP 11=RINSE ► 12=RINSE ►► 13=RINSE ►►► 20=LEAKAGE ? 21=MIX ► 22=MIX ►► 31=READY |  | I428.1 The following statuses are passed through during every step.
MENGER.START | 2320 | MIXER | Fill 0=NO 1=ALL TANKS 2=FERTILIZER-T 3=A-TANK 4=B-TANK 5=C-TANK 6=D-TANK 7=LYE-TANK 8=ACID-TANK 12=MIN FERTILIZER-T 13=MIN A-TANK 14=MIN B-TANK 15=MIN C-TANK 16=MIN D-TANK 17=MIN LYE-TANK 18=MIN ACID-TANK |  | I428 I428.1 See I428 Meststof instellingen
MENGER.TOESTAND | 2324 | MIXER | status fertilizer mixer 0=--- 1=STOP 2=REST 10=FILL TANK 11=FILL INTERMED TANK 20=INTERM TANK -> TANK 21=INTERM TANK ->DRAIN 30=ERROR 40=WAIT |  | I428 I428.1 See I428 Meststof instellingen
UniMeasurements.ValueUni | 7AA6 | CUSTOM MEAS | Uni |  | I705 The result of universal measurement, without unit.
CoBh_DosRef.DosFcoGew | 2671 | CO₂ MANAGEM | Des CO₂ production | kg CO₂/hr | M250 M250.1 Desired CO2 production for the CO2 management. This demand is determined by adding the CO2 demands from the CO2 controls. M250.2 The desired CO2 production for the CO2 management. This demand is determined by adding the CO2 demands from the CO2 controls.
CoBh_Lev.FcoGer | 2676 | CO₂ MANAGEM | Act CO₂ production | kg CO₂/hr | M250 M250.1 The actual CO2 production by the CO2 management.
CoBh_Verd.BeperkCdBer | 2686 | CO₂ MANAGEM | Limitation CO₂ production 0=NONE 1=ALTERNATIVE 2=HEAT BY-PRODUCT 3=MAX VALVES 4=MAX SOURCES 5=NUMBER ON 6=EMERGENCY STOP |  | M250
CoBh_Verd.VerdFcoMax | 2693 | CO₂ MANAGEM | Max CO₂ production | kg CO₂/hr | M250
AUS_UI_METEN.CD_AUS_TST_BER | 26D1 | EXTERNAL CO₂ | Status 0=OFF 1=DES ACTIVE 2=ACTIVE 3=ERROR |  | M260 The status of the external CO2 source.
CO2Bron_Prod.CdactBer | 26EB | EXTERNAL CO₂ | CO₂ production active 0=NO 1=YES |  | M250 M255 Indication of whether CO2 is being dosed with this source. M260 Indication whether there is CO2 dosage with the external CO2 source.
CO2Bron_Prod.FcoGer | 26EC | EXTERNAL CO₂ | CO₂ kg per hour | kg CO₂/hr | I260 The actual CO2 production of the external CO2 source. M250 M255 The actual CO2 production by this source. M260 The actual CO2 production by the external CO2 source.
CO2Bron_Vrg.FcoGew | 26F1 | EXTERNAL CO₂ | Des CO₂ production | kg CO₂/hr | I260 The CO2 demand that is requested by the CO2 management from the external CO2 source and that must be produced by the external CO2 source. M250 M255 The desired CO2 production for this source. M260 The desired CO2 production for external CO2 source, that is demanded from the CO2 management.
PULSM_CO2.FLOW | 273F | EXTERNAL CO₂ | Current consumption | unit/hour |
CoRgDosBerCo.AanpDempBer | 2824 | CO₂ DOSAGE | influence smoothing | kg CO₂/ha/hr | I170 Calculated influence of the damping on the desired CO2 dosage/concentration. M170
CoRgDosBerCo.ActDosGewBer | 282B | CO₂ DOSAGE | calculated dosage | kg CO₂/ha/hr | I170 Calculated CO2 dosage depending on the set CO2 dosage and influences. I170 Calculated CO2 dosage depending on the set CO2 dosage and influences. M170 Calculated CO2 dosage, depending on the set CO2 dosage and influences of wind speed, vent position, temperature, humidity, F&P systems, climate and crop treatment.
CoRgDosBerCo.DosGewBer | 282E | CO₂ DOSAGE | set dosage | kg CO₂/ha/hr | I170 The set CO2 dosage determined from the radiation-dependent settings of the Radiation : dosage setting table. M170 The set CO2 dosage determined from the radiation-dependent settings of the Radiation : dosage setting table (I170 CO2-programma/Strategie).
CoRgDosBerConc.CcoGew | 2837 | CO₂ DOSAGE | Set CO₂ concentration | ppm | I170 The set CO2 concentration determined from the radiation-dependent settings of the Radiation : desired concentration setting table. For the CO2 concentration, the Deviation CO₂ conc : CO₂ dos (I170.1 CO2-programma/Invloeden) setting is also of importance. M170 The set CO2 concentration determined from the radiation-dependent settings of the Radiation : desired concentration setting table (I170 CO2-programma/Strategie).
CoRgDosBerConc.CcoGewBer | 2838 | CO₂ DOSAGE | Calculated CO₂ concentration | ppm | I170 The calculated CO2 concentration, depending on the set CO2 dosage and influences of wind speed, vent position, temperature, humidity, F&P systems, climate and after possible blocking by the crop treatment. M170 The calculated CO2 concentration, depending on the set CO2 concentration and influences of wind speed, vent position, temperature, humidity, F&P systems, climate and crop treatment.
CoRgDosBerGas.ActDosGewBer | 2842 | CO₂ DOSAGE | calculated dosage | m³ gas/ha/hr | I170 Calculated CO2 dosage depending on the set CO2 dosage and influences. M170 Calculated CO2 dosage, depending on the set CO2 dosage and influences of wind speed, vent position, temperature, humidity, F&P systems, climate and crop treatment.
CoRgDosBerGas.DosGewBer | 2845 | CO₂ DOSAGE | set dosage | m³ gas/ha/hr | I170 The set CO2 dosage determined from the radiation-dependent settings of the Radiation : dosage setting table. M170 The set CO2 dosage determined from the radiation-dependent settings of the Radiation : dosage setting table (I170 CO2-programma/Strategie).
CoRgMomCo.DosTotaalBer | 2849 | CO₂ DOSAGE | actual dosage total | kg CO₂/ha/hr | M170 Actual total dosage (flow). This is the sum of Actual dosage active , Actual dosage passive and Actual dosage on-off heating (flow).
CoRgMomGas.DosTotaalBer | 284E | CO₂ DOSAGE | actual dosage total | m³ gas/ha/hr | M170 Actual total dosage (flow). This is the sum of Actual dosage active , Actual dosage passive and Actual dosage on-off heating (flow).
CoRgToest.CdBeperkKlimBew | 2852 | CO₂ DOSAGE | Climate limitation 0=NONE 1=TEMPERATURE 2=HUMIDITY 3=CONCENTRATION 4=MEAS.DEFECTIVE 5=AIR QUALITY 6=CROP TREATM. 7=FAN AIRTREATMENT |  | I170.1 M170 Indication of the limitation by the climate.
CoRgToest.ConcGem | 2854 | CO₂ DOSAGE | Measured CO₂ concentration | ppm | I170 The measured CO2 concentration. I170.1 M170 The measured CO2 concentration.
CoRgToest.ConcMaxBer | 2856 | CO₂ DOSAGE | Calc maximum CO₂ concentration | ppm | I170.1 M170
CoRgToest.DosType | 2858 | CO₂ DOSAGE | Dosage type 0=NONE 1=PASSIVE 2=ACTIVE 3=BOTH |  | M170 Selection of the type of dosage.
FanStat.CdStatBer | 28D6 | FAN | Status 0=OFF 1=ON 2=MIN TIME OFF 3=MIN TIME ON 4=NOT CONTROLLED |  | I255
CoTr_Toest.DosCcoGem | 28E8 | CO₂ TRANSP | Measured CO₂ concentration | ppm | I255 Display of the highest measured CO2 concentration of all connected CO2 controls at this moment.
PlantRefs.CropActLimitDown | 2C07 | CROP MONITOR | crop activity lower limit | % | I106 The limit below which the influences of the crop monitor control are active.
PlantRefs.CropActLimitUp | 2C08 | CROP MONITOR | crop activity upper limit | % | I106
PlantRefs.CropActSmoothed | 2C0C | CROP MONITOR | measured crop activity | % | I106 M100 The measured crop activity expressed in a percentage from 0 to 100%.
PlantRefs.CropPerfPast24h | 2C2E | CROP MONITOR | crop performance 24-hours |  | I106
DischargeProg.DischargeState | 63F5 | DISCH. WATER | Status 0=REST 1=RECIPE 2=START 3=OPERATION |  | I445 The status of the fill valve. M430 Status of the discharge program (see I445). M440 Status of the discharge program (see I445).
DRAIN_BER.ETM_DRN_PR_CONT | 2CB7 | DRAIN TRAY | 24 hours drain percentage | % | I405.1
TENSIO_M.TENSIO | 2CF9 | TENSIOMETER | Tensio | hPa | I405.1 Tension limit that is measured at this moment. M405 The average tensio (tension of the ground) per tensio meter after the 24 hour period transition. M405 The measured tensio (tension of the ground) per tensio meter.
MoistureMeas.UsedEC | 2CFE | SUBSTRATE | used EC | mS/cm | I405.1 In the event of multiple measurements, the measurement value used is shown here (average, highest or lowest, depending on the selection in I405.4). I405.4 The measured EC value in the substrate, depending on the selection of average, highest or lowest. M405 The average EC of the slab after the 24-hour transition which is measured with the substrate meter. M405 The measured EC in the substrate, measured with a substrate meter.
MoistureMeas.UsedTemperature | 2CFF | SUBSTRATE | used temperature | °C | I405.1 In the event of multiple measurements, the measurement value used is shown here (average, highest or lowest, depending on the selection in I405.4). I405.4 The measured temperature in the substrate, depending on the selection of average, highest or lowest. M405 The measured temperature in the substrate, measured with a substrate meter.
ROOTO_GEM.Indroging | 2D12 | SLAB WEIGHER | Dry-out | l/m² | I405.1 The calculated dry-out of the slab in l/m2. The dry-out is calculated by the transpiration model and a drain quantity measurement such as the Priva Irrigation Measurement. M405 The calculated dry-out of the slab in l/m2 indicates how far away the mat is from saturation. The dry-out is calculated using the transpiration model and the weight measurement of the Groscale.
ROOTO_GEM.MeasTranspRate | 7DAC | SLAB WEIGHER | Transpiration rate | l/m²/hr | I405.1 The speed of transpiration. This speed is calculated using the transpiration model and a drain quantity measurement such as the Priva Irrigation Measurement. M405 The speed of the transpiration. This speed is calculated using the transpiration model and the measurement of the Groscale. The difference between the Groscale and the standard weight measurements is the unique interface with the control software. This means minor differences can be measured reliably and from this the transpiration is deducted.
ROOTO_GEM.VerzGewicht | 2D16 | SLAB WEIGHER | Saturation weight | kg | I405.1 The weight of the saturated slab. If there is sufficient drain (more than 5%) after a cycle, the substrate is considered saturated. The weight at that moment is the saturation weight. It gives an indication of the condition of the substrate. M405 The weight of the saturated slab. If there is sufficient drain (more than 5%) after a cycle, the substrate is considered saturated. The weight at that moment is the saturation weight. It gives an indication of the condition of the substrate.
VOCHT_GEM.GEWICHT | 2D1B | SLAB WEIGHER | Weight | kg | I405.1 The measured weight of the slab. M405 The measured weight of the slab.
DRN_GEG.BEURT_DR_GEM_EC | 2D2B | MOIST MEAS | EC | mS/cm | M405 The EC drain of the last irrigation cycle.
DRN_GEG.BEURT_DR_GEM_PH | 2D2C | MOIST MEAS | pH | pH | M405 The pH drain of the last irrigation cycle.
DRN_GEG.BEURT_DRN_CONT | 2D2D | MOIST MEAS | Drain | l | M405 The measured drain quantity of a cycle. This quantity keeps on rising until the time of the next start. At the end of a cycle, after the draining period, a drain is calculated in l/m2 and a drain percentage determined from this drain quantity and the measured water dose through the water system. After a start, the quantity begins again at 0 litres.
DRN_GEG.BEURT_DRN_OPP | 2D2E | MOIST MEAS | Drain | l/m² | M405 The drain in litres per m2 of greenhouse area of the last irrigation cycle.
DRN_GEG.BEURT_DRN_PR | 2D2F | MOIST MEAS | cycle drain % | % | M405 The average drain percentage of the last irrigation cycle.
DRN_GEG.BEURT_OPN_OPP | 2D30 | MOIST MEAS | Take up | l/m² | M405 The quantity of water absorbed by the plant after the last irrigation cycle. This is calculated by subtracting the measured drain quantity from the given quantity. If a drain quantity measurement such as the Precision Irrigation Management is present, an abrupt increase or decrease in weight can also be taken into account.
DRN_GEG.BEURT_TOESTAND | 2D31 | MOIST MEAS | Status cycle drain 0=REST 1=CHECK 2=OPERATION 3=START 4=RESTART 5=IRR CYCLE 6=WAIT FOR DRAIN END 7=MEASURE |  | M405
DRN_GEG.ETM_DRN_OPP_C | 2D36 | MOIST MEAS | Drain | l/m² | M405 The drain in litres per m2 greenhouse area after the 24 hour period transition.
DRN_GEG.ETM_DRN_PR_CONT | 2D38 | MOIST MEAS | cycle drain % | % | M405 The average drain percentage after the 24 hour period transition.
DRN_GEG.ETM_OPN_OPP_C | 2D3B | MOIST MEAS | Take up | l/m² | M405 The quantity of water absorbed by the plant after the 24-hour transition. This is calculated by subtracting the measured drain quantity from the given quantity. If a drain quantity measurement such as the Precision Irrigation Management is present, an abrupt increase or decrease in weight can also be taken into account.
GIFT_GEG.BEURT_GIFT_OPP | 2D48 | MOIST MEAS | Dose | l/m² | M405 The water dose in litres per m2 of greenhouse area of the last irrigation cycle.
GIFT_GEG.ETM_GIFT_OPP_C | 2D4C | MOIST MEAS | Dose | l/m² | M405 The water dose in litres per m2 greenhouse area after the 24 hour period transition.
VOCHT_BEW.VOCHTGEHALTE_A | 2D7F | MOIST MEAS | moisture level | % | I405 The moisture level that is being monitored. This value is set in the linked start strategy. The measured moisture level is determined by means of the slab weight or a moisture level measurement. M405 The measured moisture level of the substrate, measured with a slab weigher or with a substrate meter.
EBMeasure.ActElecOffTake | 7CE1 | E-boiler | Actual electricity off-take | kW | M315 The current electricity consumption of the e-boiler.
EBMeasure.ActHeatCap | 7CE2 | E-boiler | Actual heat production | kW | M300 M315 The heat capacity currently produced by the e-boiler.
EBMeasure.ActReturnTemp | 7CE9 | E-boiler | Measured return temperature | °C | M300.1 The measured return temperature. M315 The measured return temperature.
EBMeasure.ActSupplyTemp | 7CEA | E-boiler | Measured supply temperature | °C | M300.1 The measured supply temperature. M315 The measured supply temperature.
EBMeasure.ControlStatus | 7CF4 | E-boiler | Status e-boiler control 0=NOT OPERABLE 1=OFF 2=ON 3=PRE-RUNNING 4=SHUTTING DOWN 5=COOLING DOWN |  | M300.1 See 8 Status e-boiler control . M315
EBMeasure.DesElectricCap | 7CF6 | E-boiler | Des adjustment electrical capacity | kW | M315 The desired adjustment of the capacity by the electricity management.
EBMeasure.DesExternalCap | 7CF8 | E-boiler | Des external electrical capacity | kW | M315 The desired electrical capacity, based on External capacity .
EBMeasure.DesReserveCap | 7CFA | E-boiler | Des reserve capacity | kW | M300 M315 The desired reserve capacity, based on heat management (I300).
EBMeasure.DesStorageCap | 7CFB | E-boiler | Des forced storage capacity | kW | I315.2 Desired capacity of the e-boiler that is calculated for the filling of the heat buffer in the active period. M300 M315 The desired forced storage capacity, as set in I315.2 E-boiler gedwongen opslag.
EBMeasure.SystemLimitation | 7D0E | E-boiler | Limitation 0=NONE 1=CONFIGURATION ERROR 2=INSTALLATION 3=LOCAL BLOCK 4=EMERGENCY HOLD 5=FAILURE 6=PRESSURE 7=NO FLOW 8=NOT ACTIVE 9=TEMP. TOO HIGH 10=WAIT REL 11=COOLING WATER 12=BUFFER 13=TEMP. TOO LOW |  | M300.1 See 9 Limitation . M315
EL_BEH.GEINV_VERM | 2E4D | ELECTR.MAN | Total desired electrical capacity | kW | M200 The total desired electrical capacity by all electricity consumers, whereby the switching times, delays and maximum available electrical capacity are not taken into account.
EL_BEH.GER_VERM_UI | 2E4F | ELECTR.MAN | total limited desired electrical capacity | kW | M200 The total desired electrical capacity by all electricity consumers, which is limited by the maximum available electrical capacity. The switching times and delays are taken into account.
EL_BEH.MAX_EL_VERM | 2E50 | ELECTR.MAN | Max electrical capacity | kW | M200 The maximum available electrical capacity.
ElekMomRegis.BerVeBeschikMom | 2E8E | ELECTR.MAN | Total measured electrical capacity | kW | M200 The measured total electrical capacity.
ElekMomRegis.GemVeExpMom | 2E97 | ELECTR.MAN | Measured electrical export | kW | M204 The measured electricity export.
ElekMomRegis.GemVeImpMom | 2E98 | ELECTR.MAN | Measured electrical import | kW | M204 The measured electricity import.
ElekMomRegis.GemVeProdMom | 2E99 | ELECTR.MAN | measured electricity production CHP | kW | M204 The measured electricity production by the CHP(s).
GASBEGRENS.BER_CORR_GASM | 3031 | GAS DISTR | Calc max gas consumption | m³/hr | I304 The calculated maximum gas consumption of the (external) gas strategy or external gas maximum. M304 The calculated maximum gas consumption at this applies at this moment. The maximum gas consumption can be the absolute maximum gas consumption, the maximum from the gas strategy, from the external gas strategy or a contact maximum gas consumption. This calculated maximum gas consumption is including the decrease by controlled and uncontrolled gas consumers. M304.1
GASBEGRENS.GASMETING | 303B | GAS DISTR | Measured gas consumption | m³/hr | I304 The measured gas consumption by a connected pulse meter.
GASBEGRENS.MOM_GASVERBR | 3044 | GAS DISTR | Calc gas consumption | m³/hr | I304 The calculated gas consumption based on the actual capacity and the efficiency of the active heat sources. M304.1
GEMID_GASVERBR.GER_GASSOM | 3066 | GAS DISTR | Measured gas sum | m³ | M304 The cumulated measured gas consumption in the period for the average gas consumption.
GEMID_GASVERBR.MAX_GASSOM | 306A | GAS DISTR | Maximum gas sum | m³ | M304 The cumulated maximum gas consumption in the period for the average gas consumption. This maximum gas sum depends on the length of the period and the specified (absolute) maximum gas consumption.
AirTreatment.CalcSupplyHumRat | 6D62 | ATU | Calculated supply air AH ratio | g/kg | M195 The calculated absolute air humidity ratio.
AirTreatment.CalcSupplyTemp | 6D64 | ATU | Calculated supply air temperature | °C | M195 The calculated temperature of the air that is blown into the indoor area.
AirTreatment.CoolAirHum | 6D66 | ATU | Cooling air humidity | % | M195 The humidity measurement on the outlet side of the cold block.
AirTreatment.CoolAirTemp | 6D68 | ATU | Cooling air temperature | °C | M195 The temperature measurement on the outlet side of the cold block.
AirTreatment.Fan | 6D69 | ATU | Fan 0=NO 1=YES |  | M195 The supply fan is active.
AirTreatment.FanCapacity | 6D6C | ATU | Fan capacity | % | M195 The capacity of the supply fan.
AirTreatment.FanDefect | 6D6E | ATU | Fan failure 0=NO 1=YES |  | M195.1 Failure message of the fan.
AirTreatment.FanIntervention | 6D71 | ATU | Fan intervention 0=NO 1=YES |  | M195.1 Indicates whether the control has been copied to the controller by means of an override switch.
AirTreatment.MeasSupplyHumRat | 6D73 | ATU | Measured supply air AH ratio | g/kg | M195 The measured absolute air humidity ratio.
AirTreatment.MeasSupplyHumRel | 6D74 | ATU | Measured supply air RH | % | M195 The measured air humidity
AirTreatment.MeasSupplyTemp | 6D76 | ATU | Measured supply air temperature | °C | M195 The measured temperature of the supply air.
AirTreatment.MixHumCool | 6D78 | ATU | Mixed air humidity | % | M195 The air humidity of the mixed air.
AirTreatment.MixTempCool | 6D7A | ATU | Mixed air temperature | °C | M195 The temperature of the mixed air.
AirTreatment.OuterValve | 6D7C | ATU | Outside damper position | % | M195 The valve position of the outside air section.
AirTreatment.OuterValveDefect | 6D7F | ATU | Outside damper error 0=NO 1=YES |  | M195.1 A error message has been detected.
AirTreatment.OuterValveInter | 6D81 | ATU | Outside damper intervention 0=NO 1=YES |  | M195.1 Indicates whether the control has been copied to the controller by means of an override switch.
AirTreatment.PumpCool | 6D83 | ATU | Cooling pump active 0=NO 1=YES |  | M195 The cooling pump is active.
AirTreatment.PumpCoolCap | 6D85 | ATU | Cooling pump capacity | % | M195 The capacity of the cooling pump.
AirTreatment.PumpHeat | 6D8B | ATU | Heating pump active 0=NO 1=YES |  | M195 The heating pump is active.
AirTreatment.PumpHeatCap | 6D8D | ATU | Heating pump capacity | % | M195 The capacity of the heating pump.
AirTreatment.PumpHeatDefect | 6D8F | ATU | Heating pump failure 0=NO 1=YES |  | M195.1 A error message has been detected.
AirTreatment.PumpHeatInter | 6D93 | ATU | Heating pump intervention 0=NO 1=YES |  | M195.1 Indicates whether the control has been copied to the controller by means of an override switch.
AirTreatment.RecircValve | 6D97 | ATU | Recirculation damper position | % | M195 The valve position of the recirculation section.
AirTreatment.RecircValveDef | 6D99 | ATU | Recirculation damper error 0=NO 1=YES |  | M195.1 A error message has been detected.
AirTreatment.RecircValveInter | 6D9C | ATU | Recirculation damper intervention 0=NO 1=YES |  | M195.1 Indicates whether the control has been copied to the controller by means of an override switch.
AirTreatment.ReturnTempCool | 6D9E | ATU | Cooling return water temperature | °C | M195 The temperature of the return water for the cooling.
AirTreatment.ReturnTempHeat | 6DA0 | ATU | Heating return water temperature | °C | M195 The temperature of the return water for the heating.
AirTreatment.SupplyTempCool | 6E21 | ATU | Cooling supply water temperature | °C | M195 The temperature of the supply water for the cooling.
AirTreatment.SupplyTempHeat | 6E24 | ATU | Heating supply water temperature | °C | M195 The temperature of the supply water for the heating.
AirTreatment.ValveCoolDefect | 6E29 | ATU | Cooling valve error 0=NO 1=YES |  | M195.1 A error message has been detected.
AirTreatment.ValveCoolInter | 6E2B | ATU | Cooling valve intervention 0=NO 1=YES |  | M195.1 Indicates whether the control has been copied to the controller by means of an override switch.
AirTreatment.ValveCoolPos | 6E2F | ATU | Cooling valve position | % | M195 The valve position of the cooling.
AirTreatment.ValveHeatDefect | 6E32 | ATU | Heating damper failure 0=NO 1=YES |  | M195.1 A error message has been detected.
AirTreatment.ValveHeatInter | 6E35 | ATU | Heating damper intervention 0=NO 1=YES |  | M195.1 Indicates whether the control has been copied to the controller by means of an override switch.
AirTreatment.ValveHeatPos | 6E39 | ATU | Heating valve position | % | M195 The valve position of the heating.
CurrentStratVal.CO2 | 6DB6 | Indoor CMP | CO₂ | ppm | I195
CurrentStratVal.HumRatDef | 6DBA | Indoor CMP | Humidity ratio deficit | g/kg | I195
CurrentStratVal.HumRel | 6DBD | Indoor CMP | RH | % | I195
CurrentStratVal.Light | 6DC1 | Indoor CMP | Light level | % | I195
CurrentStratVal.Light2 | 6DC4 | Indoor CMP | Light level 2 | % | I195
CurrentStratVal.Light3 | 6DC6 | Indoor CMP | Light level 3 | % | I195
CurrentStratVal.Light4 | 6DC9 | Indoor CMP | Light level 4 | % | I195
CurrentStratVal.Light5 | 711C | Indoor CMP | Light level 5 | % | I195
CurrentStratVal.Light6 | 711D | Indoor CMP | Light level 6 | % | I195
CurrentStratVal.Pressure | 6DCD | Indoor CMP | Pressure difference | Pa | I195
CurrentStratVal.Temp | 6DF1 | Indoor CMP | Temperature | °C | I195
ExtraMeas.AbsHumRat | 6DF6 | ExtrMeas | Absolute humidity ratio | g/kg | M195.2
ExtraMeas.AirTemp | 6DFA | ExtrMeas | Air temperature | °C | M195.2
ExtraMeas.GasMeas | 6E00 | ExtrMeas | Gas measurement | ppm | M195.2
ExtraMeas.HumRel | 6E04 | ExtrMeas | RH | % | M195.2
ExtraMeas.Intervention | 6E07 | ExtrMeas | Intervention 0=NO 1=YES |  | M195.2
ExtraMeas.Percentage | 6E0B | ExtrMeas | Percentage | % | M195.2
ExtraMeas.Pressure | 6E0F | ExtrMeas | Pressure difference | Pa | M195.2
ExtraMeas.State | 6E31 | ExtrMeas | Status 0=OFF 1=ON |  | M195.2
ExtraMeas.Temp | 6E34 | ExtrMeas | Temperature | °C | M195.2
ExtraMeas.WaterTemp | 6E37 | ExtrMeas | Water temperature | °C | M195.2
CO2AndPurging.Intervention | 6E09 | Indoor CMP | Intervention 0=NO 1=YES |  | M195.1 Indicates whether the control has been copied to the controller by means of an override switch.
CO2AndPurging.Status | 6E18 | Indoor CMP | Status 0=OFF 1=ON |  | M195
CO2AndPurging.ValveError | 6E1B | Indoor CMP | Valve/damper error 0=NO 1=YES |  | M195.1 A error message has been detected for the valve.
CO2AndPurging.ValvePos | 6E1F | Indoor CMP | Valve position | % | M195 Valve position of the CO₂ supply and air exhaust.
Lighting.Defect | 6DCC | Grow Light | Failure 0=NO 1=YES |  | M195.2
Lighting.Intervention | 6DD0 | Grow Light | Intervention 0=NO 1=YES |  | M195.2
Lighting.Level | 6DD4 | Grow Light | Light level | % | M195.2
Lighting.State | 6DE8 | Grow Light | Status 0=OFF 1=ON |  | M195.2
MeasPoint.CO2 | 6DA3 | MP | CO₂ | ppm | M195 The measured CO₂ concentration of the measuring box.
MeasPoint.HumRatDef | 6DA5 | MP | Humidity ratio deficit | g/kg | M195 The humidity ratio deficit calculated using the temperature and the relative air humidity.
MeasPoint.HumRatio | 6DA6 | MP | Absolute humidity ratio | g/kg | M195 The absolute moisture level calculated using the temperature and the relative air humidity.
MeasPoint.HumRel | 6DA8 | MP | RH | % | M195 The measured relative air humidity of the measuring box.
MeasPoint.Temperature | 6DBE | MP | Temperature | °C | M195 The measured temperature of the measuring box.
UnivMeas.MeasA | 6D90 | Univ Meas | Measurement A |  | M195.2
UnivMeas.MeasB | 6D92 | Univ Meas | Measurement B |  | M195.2
UnivMeas.MeasC | 6D95 | Univ Meas | Measurement C |  | M195.2
UnivMeas.MeasD | 6D98 | Univ Meas | Measurement D |  | M195.2
ExternalAlarms.HighAlarm | 6D6F | Indoor CMP | High alarm 0=NO 1=YES |  | I195.1 Indicates whether a high priority/low priority/Priva Office alarm is active. The High/Low alarm is an alarm in the Top Control project. The Priva Office alarm is an alarm in the Indoor growing strategy.
ExternalAlarms.LockedAlarm | 6D70 | Indoor CMP | Locked alarm active 0=NO 1=YES |  | I195.1
ExternalAlarms.LowAlarm | 6D72 | Indoor CMP | Low alarm 0=NO 1=YES |  | I195.1 Indicates whether a high priority/low priority/Priva Office alarm is active. The High/Low alarm is an alarm in the Top Control project. The Priva Office alarm is an alarm in the Indoor growing strategy.
ExternalAlarms.POAlarm | 6D75 | Indoor CMP | Priva Office alarm 0=NO 1=YES |  | I195.1 Indicates whether a high priority/low priority/Priva Office alarm is active. The High/Low alarm is an alarm in the Top Control project. The Priva Office alarm is an alarm in the Indoor growing strategy.
LightCommonData.Blocked | 6D80 | Indoor CMP | Growing light blocked external 0=NO 1=YES |  | M195.2 The Indoor control blocks the lighting, e.g. because the temperature is too high.
Setpoint.InterventCO2 | 6D84 | Indoor CMP | CO₂ intervention 0=NO 1=YES |  | M195.1
Setpoint.InterventHumid | 6D86 | Indoor CMP | Humidity intervention 0=NO 1=YES |  | M195.1
Setpoint.InterventLight | 6D89 | Indoor CMP | Light intervention 0=NO 1=YES |  | M195.1
Setpoint.InterventPress | 6D8A | Indoor CMP | Pressure intervention 0=NO 1=YES |  | M195.1
Setpoint.InterventTemp | 6D8C | Indoor CMP | Temperature intervention 0=NO 1=YES |  | M195.1
BRAND_STAT.BRAND_TOEST | 3173 | BOILER | Burner status 0=DISCONN 1=OFF 2=ON 3=HF-LS 4=HF-HS 5=CO₂ POS 6=LOW SP 7=HIGH SP 8=NO RELEASE 9=WAIT REL 11=ERROR 12=WAIT REL |  | I310 Status of the burner. M250.1 The status of the burner. See M300.1 HT-warmtebeheer - HT-bronnen. M300.1 The status of the burner. M310 Modulating burners:
BRAND_STAT.GER_BRAND_VERM | 3175 | BOILER | actual capacity | kW | M300 The actual heat capacity by the boiler. M310 M310 The actual capacity of the switching burner.
BRAND_STAT.GER_GASKL_ST | 3176 | BOILER | actual valve position | % | M310
CO2ktl_Prod.CdactBer | 3191 | BOILER | CO₂ production active 0=NO 1=YES |  | M250 M310.1 Indication whether there is CO2 dosage with the boiler.
KETEL.BEPERKING | 31ED | BOILER | Limitation boiler 0=NONE 1=EXTERN. BLK 2=COOLING WATER 3=GAS LIMITATION |  | I310 M310
KETEL.BER_KET_TEMP | 31EE | BOILER | calculated boiler temperature | °C | I310 M310
KETEL.GEW_CO2_VERM | 31FD | BOILER | desired CO₂ capacity | kW | M300 The desired CO2 capacity of the boiler, that is dependent on the set minimum, maximum and absolute maximum CO2 capacity, the CO2 buffer influence and the calculated CO2 dosing capacity (refer to I310.2 Boiler/Forced storage). M310 The desired CO2 capacity of the boiler, that is dependent on the specified minimum, maximum and absolute maximum CO2 capacities, the CO2 buffer influence and the calculated CO2 dosage capacity (refer to I310.1 Boiler/Influences).
KETEL.GEW_CONS_VERM | 31FE | BOILER | desired greenhouse capacity | kW | M300 The greenhouse capacity that is allocated to the boiler. M310 The desired heat capacity because of a capacity demand from the compartments that have been allocated to this boiler.
KETEL.GEW_OPSLAG_VERM | 31FF | BOILER | Des forced storage capacity | kW | I310.2 Desired capacity of the boiler that is calculated for the filling of the heat buffer in the active period. See Gedwongen opslag in warmtebuffer. M300 The desired storage capacity of the boiler if the buffer strategy demands this (refer to M310 Boiler/Overview). M310 The required storage capacity of the boiler if the buffer strategy demands this (refer to I300 Heat management/Strategy and I310.2 Boiler/Forced storage).
KETEL.GEW_RESERV_VERM | 3200 | BOILER | Des reserve capacity | kW | M300 The required reserve capacity of the boiler if the heat reserve demands this. The heat reserve demands a capacity to meet the expected future heat demand. M310 The required reserve capacity of the boiler if the heat reserve demands this. The heat reserve demands a capacity to be able to meet an expected future heat demand.
KETEL.GEW_RETOUR_VERM | 3201 | BOILER | desired return capacity | kW | M310
KETEL.GEW_WARMTE_VERM | 3202 | BOILER | Des heating capacity | kW | M300 The desired heat capacity of the boiler, which is the sum of the demanded capacity from the greenhouse, the calculated internal capacity and the calculated return capacity (refer to M310 Boiler/Overview). M310 The desired heat capacity of the boiler, which is the sum of the capacity demanded by the greenhouse, the calculated internal capacity and the calculated return capacity (refer to M310 Boiler/Overview).
KETEL.INT_WARMTE_VERM | 3207 | BOILER | desired intern capacity | kW | M310
KETEL.KET_AFN_BEP | 3208 | BOILER | off-take limitation percentage | % | M310 Percentage limitation of the heat off-take by the heating and transport systems.
KETEL.KET_VERN_VRIJG | 320A | BOILER | Heat surplus% | % | M300.1 The heat surplus percentage of the boiler. If the boiler becomes too hot due to a forced demand, the heat surplus percentage increases. M310 The heat surplus percentage that is present with this boiler.
KETEL_.GEM_KETA_TEMP1 | 3222 | BOILER | measured boiler temperature | °C | I310 M300.1 The measured boiler temperature. M310
MOD_BRAND.BerGewBrandVerm | 3274 | BOILER | desired burner capacity | kW | M310 M310 The burner capacity that is demanded from the burner by heat management, CO2 management or for storage capacity.
MOD_BRAND.BerStapBrandVerm | 3275 | BOILER | calculated burner capacity | kW | M310
ClimateArea.AreaTempHighVal | 3344 | CLIMATE | temperature highest | °C | I12
ClimateArea.AreaTempLowVal | 3346 | CLIMATE | temperature lowest | °C | I12
ClimateArea.BalanceTempVal | 3349 | CLIMATE | temperature balance | °C | I12
KRAAN.AFWIJKING | 341F | VALVE | Deviation | % | M412 The deviation in percentages between the average measured flow and the average calculated flow of the valve. For the calculated flow the Correction more valves in (I430.1 Water system/Settings) has been taken into account. A positive deviation means that the measured flow was greater than the calculated flow.
KRAAN.FLOW | 3428 | VALVE | Flow | m³/hr | M412 The average measured flow of this valve.
KRAAN.GEMID_EC | 342C | VALVE | A_EC | mS/cm | M412 The average EC value.
KRAAN.GEMID_PH | 342D | VALVE | A_pH | pH | M412 The average pH value.
KRAAN.KR_EENH_VERBR | 3438 | VALVE | amount of water per unit | ml | M412 The water consumption per set unit.
KRAAN.KRAAN_AANWEZIG | 343A | VALVE | 0=NO 1=YES |  |
KRAAN.KRAAN_TOESTAND | 343E | VALVE | Status 0=REST 1=RECIPE 2=START 3=IRRIG 4=STAND TIME 5=RECIPE SIPH 6=STARTSIPH 7=SIPHON 8=ERROR 9=WAIT 10=RETURN 11=RECIPER 12=START R 13=RINSE 14=RUN TIME |  | I412 I412.1 Indication of the status of the valve. See I412 Kraan start, stop en reset. I414 See Status in I412 Kraan start, stop en reset. M411 The status of the valve, see I412 Kraan start, stop en reset.
KRAAN.REG_GEG | 3447 | VALVE |  |  |
KRAAN.TODOH_KRAANVAK | 3459 | VALVE | amount of water per valve | l | M411
KRAAN.VERBRUIK | 345F | VALVE | Quantity | l | M412 The total water consumption of this valve.
KRAAN.VERBRUIKM2 | 3461 | VALVE | Liters per m² | l/m² | M412 The total water consumption of this valve in l/m2.
LBS_Metingen.RVKasGemGed | 36F1 | ATU STRAT | Measured RH | % | I15 I15.1 I15.1 M15.1
LBS_Metingen.TKasGemGed | 36F2 | ATU STRAT | measured cooling temperature | °C | I15 I15.1 I15.1 M15.1
LBS_Periode.RvBevoGew | 3704 | ATU STRAT | Humidify level | % | I15 calculated humidity level at which the ATU is allowed to start humidifying the greenhouse air M15.1 humidity level at which the ATU is allowed to start humidifying the greenhouse air M15.2 humidity level at which the ATU is allowed to start humidifying the greenhouse air
LBS_Periode.RvOntvoGew | 3705 | ATU STRAT | Dehumidification level | % | I15 calculated humidity level at which the ATU is allowed to start dehumidifying the greenhouse air M15.1 humidity level at which the ATU is allowed to start dehumidifying the greenhouse air M15.2 humidity level at which the ATU is allowed to start dehumidifying the greenhouse air
LBS_Periode.TKoelGew | 3706 | ATU STRAT | cooling temperature | °C | I15 M15.1 temperature at which the ATU is allowed to start cooling the greenhouse air
LBS_Periode.TVerwGew | 3707 | ATU STRAT | heating temperature | °C | I15 M15.1 temperature at which the ATU is allowed to start heating the greenhouse air
GEN_STU_UI_01.CD_BEPERKING | 37F2 | ATU | Limitation 0=NONE 1=ERROR 2=I/O DEFECT 3=I/O ASSIGN. 4=MANUAL 5=MIN LIMIT 6=MAX LIMIT 7=ACT TIME-OUT 8=ANTI STUCK PROTECT 9=RELEASE |  | I157 I158 M157 M158 M158
GEN_STU_UI_01.PERC_STU_GEM | 37FD | ATU | Measured position | % | I157 measured position of the inlet or the air outlet I158 measured position of the inlet or air outlet M157 measured position of the mixing chamber inlet or the air outlet M158 measured position of the inlet M158 measured position of the air outlet
GEN_STU_UI_01.PERC_STU_GEW | 37FE | ATU | Desired position | % | I157 The desired position of the inlet or the air outlet. This position is calculated based on the maximum and minimum mixing ratio and the damped mixing ratio (see Maximum mixing ratio , Minimum mixing ratio and Calculated smoothed mixing ratio ). I158 The desired position of the inlet or air outlet. This position is calculated based on the maximum and minimum mixing ratio and the smoothed mixing ratio (see Maximum mixing ratio , Minimum mixing ratio and Calculated smoothed mixing ratio in I157). M157 The desired position of the mixing chamber inlet or the air outlet. This position is calculated based on the maximum and minimum mixing ratio and the smoothed mixing ratio (see Maximum mixing ratio , Minimum mixing ratio and Calculated smoothed mixing ratio in Strategie). M158 Desired position of the inlet M158 The desired position of the air outlet. This position is calculated based on the maximum and minimum mixing ratio and the smoothed mixing ratio (see Maximum mixing ratio , Minimum mixing ratio and Calculated smoothed mixing ratio in I157).
MENGKLEP_IN.T_MK_GEW | 38A8 | ATU | Calc supply temperature | °C | M155 calculated temperature of the water flowing into the block M155 calculated temperature of the water flowing into the block
LB_FAN_MREF.AVKasGem | 3CC4 | ATU | absolute humidity blow-out | g/m³ | M153 measured AH of the airflow
LB_FAN_MREF.RVKasGem | 3CCB | ATU | relative humidity blow-out | % | M153
LB_FAN_MREF.TKasGem | 3CCC | ATU | blow-out temperature | °C | M153 measured temperature of the airflow
LB_OUT_FAN_GROEP.BerMaxPercBasis | 3D2E | ATU | total maximum fan capacity | % | I153 Control area of the fan capacity if Release increase fan capacity has been released. If there is no deviation between the desired and the measured value, the minimum fan capacity applies. If the deviation between the desired and the measured value is greater than or equal to the set P band, the maximum fan capacity applies.
LB_OUT_FAN_GROEP.BerMinTotaal | 3D30 | ATU | total minimum fan capacity | % | I153 Control area of the fan capacity if Release increase fan capacity has been released. If there is no deviation between the desired and the measured value, the minimum fan capacity applies. If the deviation between the desired and the measured value is greater than or equal to the set P band, the maximum fan capacity applies.
LB_OUT_FAN_GROEP.FFanBer | 3D4E | ATU | Calculated flow fan | m³/hr | M150.1 The calculated quantity of air that is displaced by the fan or fans of the same ATU. This quantity is calculated on the basis of the Calculated flow inlet grh air (M153) and Calculated flow inlet outside air (M153) that flow into the mixing chamber. M153 The calculated quantity of air that is displaced by the fan or fans of the same ATU. This quantity is calculated based on the calculated amount of greenhouse air and of outside air flowing into the mixing chamber.
LB_OUT_FAN_GROEP.FFanGer | 3D54 | ATU | actual flow fan | m³/hr | M150.1 actual quantity of air that has been displaced by the fan or fans of the same ATU M153 actual quantity of air that is displaced by the fan or fans of the same ATU
LB_OUT_FAN_GROEP.PercFanBer | 3D64 | ATU | calculated fan capacity | % | I153 I153.2 M150.1 This capacity is calculated on the basis of the desired capacity of the fan (I153) plus any increase ( Calc increase cap by temp difference in I153). M153
LB_OUT_FAN_GROEP.PercFanGer | 3D65 | ATU | actual fan capacity | % | I153 I153.1 I153.2 M150.1 The current position of the blow-out fan. M153
LB_OUT_FAN_GROEP.PercFanGew | 3D66 | ATU | desired fan capacity | % | I153 I153 I153.1 I153.2 M153
MaxUitblaasT.IngMaxUitblaasT | 3E12 | ATU | Maximum blow-out temperature | °C | I151 Maximum blow-out temperature is set above
MaxUitblaasT.T_BasisSLangGew | 3E13 | ATU | unlimited maximum blow-out temperature | °C | I151
MaxUitblaasT.TMaxUitblBer | 3E15 | ATU | limited maximum blow-out temperature | °C | I151
MinUitblaasT.CdjnActief | 3E56 | ATU | Blow-out strategy active 0=NO 1=MINIMUM 2=MIN COOL 3=MAXIMUM |  | I150
MinUitblaasT.GewMinUitbltemp | 3E63 | ATU | limited minimum blow-out temperature | °C | I150
MinUitblaasT.T_BasisSLangGew | 3E69 | ATU | unlimited minimum blow-out temperature | °C | I150
LogDevUI.CalcPosition | 73DA | AIR CIRCUL. | Calculated position | % | I190.3 The position to be achieved. M190 The position to be achieved. M192 The position to be achieved.
LogDevUI.MeasPosition | 73DB | AIR CIRCUL. | Measured position | % | I190.3 The measured position. M190 The measured position. M192 The measured position.
PosCntr.DriveState | 73DC | AIR CIRCUL. | Status 0=IDLE 1=DEACTIVATED 2=PENDING 3=ACTIVE 4=AT MAXIMUM 5=RUNNING UP 6=AT POSITION 7=RUNNING DOWN 8=AT MINIMUM 9=STOPPING |  | I190.3 The current state of the fan/air mixer. See Status M190 The current state of the fan/air mixer. See State M192 The current state of the fan/air mixer. See Status
Luchtcirculatie.ToestandVentUI | 40C4 | AIR CIRCUL. | Status air circulation control 0=OFF 1=ON 2=MIN T ON 3=MIN T OFF |  | I190 M190 See 19 Status air circulation control . M192 See 19 Status air circulation control .
MeMstPARSomRef.PARRefSomBer | 417B | PAR SENSOR | PAR sum today | mol/m² | M4 The sum of the smoothed PAR from today, counting from the Time sunrise until now.
PARMe.PARGem | 418C | PAR SENSOR | PAR | umol/s/m² | M4 M105.1 The measured PAR.
WthrRadCopy.CtrlRadiation | 41F6 | RAD SENS | radiation | W/m² | M4 M100 The measured radiation.
WthrRadCopy.MeasRadiation | 41F1 | RAD SENS | radiation measured | W/m² | M4
WthrRadCopy.RadSumToday | 41F8 | RAD SENS | radiation sum today | J/cm² | M4 The measured sum of the smoothed radiation for today, counted from Time sunrise to now. M100 The measured radiation sum counted from the moment of sunrise (M4 Overzicht/Metingen).
WthrStation.MeasRainQuantity | 6FDB | STATION | Rain quantity | mm/min | M4.2 The measured rain quantity per weather station.
WthrStation.MeasRainState | 6FDC | STATION | Rain 0=NO 1=YES |  | M4.2 Indication of whether the result of the rain measurement is active per weather station.
EL_VOCHT.BER_ABSVO | 4270 | WEATHER |  | g/m³ |
EL_VOCHT.MeasEnthalpy | 6378 | WEATHER |  | kJ/kg |
WthrObserv.CalcEnthalpyOuts | 6FBF | WEATHER | Enthalpy of outside air | kJ/kg | M4 The calculated enthalpy of the outside air based on the measured air humidity and temperature.
WthrObserv.CalcOutsAbsHum | 7009 | WEATHER | absolute humidity | g/m³ | M4 The measured absolute humidity of the outside air. M100 The measured absolute air humidity outside.
WthrObserv.CalcOutsHumDef | 427F | WEATHER | humidity deficit | g/m³ | M4 The measured humidity deficit of the outside air. M100 The measured humidity deficit outside.
WthrObserv.CalcSkyTemp | 42FC | WEATHER | Sky temperature | °C | M4 The measured sky temperature.
WthrObserv.CalcWindChillT | 42A0 | WEATHER | Calculated windchill | °C | M4 The wind chill is a measure of the quantity of heat that a body loses at the measured outside temperature and wind speed. The wind chill is calculated at an outside temperature below 10°C and with a wind speed higher than 1 m/s. At an outside temperature above 10°C and with a wind speed below 1 m/s, the calculated wind chill is equal to the measured outside temperature. The radiation and the air humidity have no influence in the calculation on the calculated wind chill.
WthrObserv.CtrlCO2Conc | 4293 | WEATHER | Outside CO₂ concentration control | ppm | M4 M4 The measured CO₂ level of the outside air.
WthrObserv.CtrlIrradiation | 42FD | WEATHER | irradiation | W/m² | M4 M100 The measured irradiation.
WthrObserv.CtrlOutsideTemp | 42A9 | WEATHER | outside temperature | °C | M4 M100 The measured outside temperature.
WthrObserv.CtrlRainPercent | 427C | WEATHER | rain percentage control | % | M4
WthrObserv.CtrlWindAngle | 42AB | WEATHER | wind direction control | ° | M4
WthrObserv.CtrlWindSpeed | 42AD | WEATHER | wind speed | m/s | M4 M100 The measured wind speed.
WthrObserv.FrostActive | 42F0 | WEATHER | frost 0=NO 1=1--- 2=-2-- 3=12-- 4=--3- 5=1-3- 6=-23- 7=123- 8=---4 9=1--4 10=-2-4 11=12-4 12=--34 13=1-34 14=-234 15=1234 |  | M4 M100 Indication whether it is freezing and if so, which frost limit is active. These can be several frost limits.
WthrObserv.MeasOutsideTemp | 429D | WEATHER | Outside temperature | °C | M4
WthrObserv.MeasOutsRelHum | 427E | WEATHER | outside humidity RH measurement | % | M4
WthrObserv.MeasRainQuantity | 42C0 | WEATHER | Rain quantity | mm/min | M4 The measured rain quantity in mm/min.
WthrObserv.RainActive | 42EE | WEATHER | rain 0=NO 1=YES |  | M4 M100 Indication whether (forced) rain is active.
WthrObserv.StormActive | 42EF | WEATHER | storm 0=NO 1=1--- 2=-2-- 3=12-- 4=--3- 5=1-3- 6=-23- 7=123- 8=---4 9=1--4 10=-2-4 11=12-4 12=--34 13=1-34 14=-234 15=1234 |  | M4 M100 Indication whether there is a storm and if so, which storm limit is active. These can be several limits.
WthrObserv.SunHeightNow | 425A | WEATHER | Sun height now | ° | M4 Current calculated angle at which the solar radiation strikes the earth’s surface. The heating control, ventilation control and light control may take the height of the sun into account
WthrObserv.WindSection | 429B | WEATHER | wind direction 0=N 1=NE 2=E 3=SE 4=S 5=SW 6=W 7=NW |  | M4 The measured wind direction. M100 The measured wind direction.
LogDevUI.MeasPosition | 76CE | Channel | Measured position | % | I208 I208.3 The measured position.
ModLightMeasure.ActRecipeNumber | 7BC6 | MOD. LIGHT | Recipe number |  | M208 The active recipe number.
ModLightMeasure.DesLightPerc | 7AB7 | MOD. LIGHT | Des. light% | % | M208 The desired light percentage of the modulating growing light system.
ModLightMeasure.DesNrOfSteps | 7AB8 | MOD. LIGHT | Des. steps |  | M208 The requested number of growing light steps for electricity off-take.
ModLightMeasure.SystemLimitation | 76E2 | MOD. LIGHT | Limitation 0=NONE 1=INSTALLATION 2=NOT OPERABLE 3=LOCAL BLOCK 4=EMERGENCY HOLD 5=WAIT HEATING 6=WAIT CURTAIN 7=WAIT REL 8=FIXED POSITION 9=CROP TREATM. 10=FORCED ON 11=FORCED OFF 12=RECIPE 13=AT MAXIMUM 14=AT MINIMUM 15=MINIMUM OFF-TAKE 16=NO STRATEGY 17=OFF DELAY |  | I208 The limitation for the modulating growing light system. M208 See 13 Limitation .
PARRegGrLiStap.GrLiStapToestCd | 469E | LIGHT STEP | Status growing light step 0=OFF 1=ON 2=WAIT ON 3=WAIT OFF |  | M20
PARRegSchKop.SchermStandGer | 46B1 | CURTAIN | Calculated shading position | % | M20 Calculated position of the shading curtain.
PARRegSchKop.SchermToestCd | 46B4 | CURTAIN | Status shading 0=OPEN 1=MINIMUM 2=CONTROL 3=CLOSE 4=WAIT OPEN |  | M20
PARCalcSetpoint.ParRegSet | 6928 | LIGHT CNTRL | Set PAR | umol/s/m² | M20 Set PAR value from the current period or correction setting.
PARRegelingAlg.CalcLightPerc | 79F3 | LIGHT CNTRL | Calculated light percentage | % | M20 The calculated light percentage from the calculated PAR value, if necessary adjusted by the decrease based on the measured light and PAR correction and limited to the calculated maximum light percentage.
PARRegelingAlg.CalcParLighting | 46E9 | LIGHT CNTRL | Calculated PAR lighting | umol/s/m² | I20
PARRegelingAlg.CalcParShading | 46F3 | LIGHT CNTRL | Calculated PAR shading | umol/s/m² | I20
PARRegelingAlg.CalcParSum | 46FA | LIGHT CNTRL | Calculated PAR sum | mol/m² | I20 M20 The Calculated PAR sum is based on the set Desired PAR sum (I20) and adjusted by all the calculated influences. This value determines whether the growing light switches off or remains off and controls the position of the shading curtains.
PARRegelingAlg.InflLiRefOnLiP | 79F5 | LIGHT CNTRL | Influence light reference | % | M20 The influence on the light percentage, based on the specified reference measurement (I20.4) and PAR reference : decrease light% or Rad. reference : decrease light% (I20.2).
PARRegelingAlg.InflParCorrOnLiP | 7B4C | LIGHT CNTRL | Influence PAR correction | % | M20 The PAR correction ensures that the calculated light percentage goes to the desired PAR value. The PAR correction depends on the specified reference measurement (I20.4), the calculated added PAR output by the growing light system, the specified PAR correction factor (dealer setting) and the option Use PAR correction for light% (I20.4).
PARRegelingAlg.ParRegLimitCd | 46F0 | LIGHT CNTRL | limitation 0=NOT PRESENT 1=MEASUREMENT 2=PAR SUM 3=EXT LIGHT 4=EXT SHADING 5=REFERENCE 6=GR. LIGHT 7=SHADING 8=INSTALLATION 9=NONE |  | M20
PARRegelingAlg.ParRegStateCd | 46F2 | LIGHT CNTRL | status 1=OFF 2=NIGHT 3=SHADING 4=LIGHT 5=ACTIVATED |  | M20
PARRegReferentie.ParGebruikt | 4709 | LIGHT CNTRL | applied PAR | umol/s/m² | I20.4 Measured PAR used by the light control to calculate the number of growing light steps and the light percentage. M20 Measured PAR used by the light control to control the position of the shading curtains and to switch the growing light on and off.
PARRegReferentie.ParSomVandaag | 470E | LIGHT CNTRL | PAR sum today | mol/m² | M20
PARRegReferentie.RadGebruikt | 7A0C | LIGHT CNTRL | Used radiation | W/m² | I20.4 Measured radiation used by the light control to calculate the number of growing light steps and the light percentage. M20 Measured radiation used by the light control to control the position of the shading curtains and to switch the growing light on and off.
PARRegSchFunc.SchStralBeperBer | 471C | LIGHT CNTRL | Actual radiation limitation | % | M20 Calculated limitation of the radiation by all closed shading curtains.
METERSTAND.METERSTAND | 4750 | ENER.PULSE M | Meter reading |  |
METERSTAND.VerbruikVd | 4756 | ENER.PULSE M | Total |  |
PULSMETER.FLOW | 4764 | ENER.PULSE M | Current consumption | unit/hour |
COM_DOS_RCPT.REGEL_EC | 47AB | RECIPE | Calculated EC | mS/cm | I403 Calculated EC value; the desired EC with the radiation decrease of the EC and the measured EC of the supply water if Toevoegen EC in I403.1 Recept/Waterbehandeling is set to YES.
RETOUR.BESTEM_SILO | 481D | RETURN | Tank |  | M440
RETOUR.BESTEM_TYPE | 481E | RETURN | Destination 0=OUTLET 1=TANK 2=ALT OUTLET 3=ALT TANK |  | M440 The destination of the return water.
RETOUR.TOESTAND | 4837 | RETURN | Status return 0=REST 1=ON-GOING 2=BUSY 3=RETURN 4=DELAY CLEANING 5=CLEANING |  | I443 Status indication of the return main. M440 The status of the return main.
SILOVK.ACTIE | 4850 | FILL VALVE | Action 0=NONE 1=FILL UP 2=FILL UP% 3=FILL TO MAX 4=FILL TO MAX% 5=ALWAYS 6=STORE |  | I440 Indication of the action of the fill valve.
SILOVK.BEPERKING | 4852 | FILL VALVE | Limitation 0=NONE 1=CALIBRATE LEVEL 2=MAX CONTENT 3=LEVEL SENSOR 4=RECYCLE TANK 5=FRESH WATER TANK 6=CONSUMPTION MAX 7=CONSUMPTION MIN 8=CONSUMPTION ZERO |  | I440 The limitation of the fill valve.
SILOVK.TOESTAND | 485D | FILL VALVE | Status 0=REST 1=RECIPE 2=START 3=FILL 4=ERROR |  | I440 The status of the fill valve. M430 The status of the tank fill valve. M440 Status of this fill valve.
TankStatusCopy.WATER_NIV | 68A0 | TANK | Water level | % | I440 Percentage of water level of the tank. A trend is also displayed. M430 See Water level in I440 Silo/Instellingen. M440 The water level in the tank as a percentage. A trend is also displayed. M440.1 The measured water level in percentages and the trend of this in the tank.
TankStatusCopy.WATER_STAND | 68A1 | TANK | Water state 0=--- 1=FULL 2=ENOUGH 3=FILL TO MAX 4=DOSING 5=FILL UP 6=BLOCK 7=BLOCK/FILL UP 8=EMPTY |  | I440 Water state in the tank. See M440 Overzicht silo. M430 The water state in the tank. M440 Water state in the tank.
START_VOORW.START_VOORW | 4AF2 | # | start cause 0=NONE 1=TEMP 2=HUMIDITY 3=RADIATION 4=RADSUM+DR 5=CLOCK 6=EXTERNAL 7=MAX REST 8=MANUAL 9=TRANSPIRATION 10=MOIST%-SLAB 11=TENSIO 12=START SEQUENCE 13=VPD SUM 14=DRY-OUT 15=TRANSPIRATION SUM 16=PAR 17=PAR-SUM+DR |  | M400 The cause for starting the irrigation. M400.2 The cause for starting the irrigation. See M400 Autostart/Actueel
STARTMGRB.START_NUM | 4B01 | # | Cycle |  | M400 This indicates the cycle number of the irrigation cycle. The number sequence is per day from 1 up to the number of cycles run on that day.
STRAL_ST.GEC_STRALSOM | 4BD5 | START PRG | radiation sum limit | J/cm² | M400
STRAL_ST.STRALSOM | 4BD8 | START PRG | radiation sum | J/cm² | M400
VERDAMP_ST.BER_DRAIN_PRC | 4BF8 | START PRG | desired drain% | % | M400 The quantity increase ensures that the desired drain percentage is increased. This allows a possible shortage to be made up for.
STRT_IRRIG.MEASDRYOUT_UNIT | 6648 | SUBSTR START | Dry-out | ml/unit | M500 The dry-out of the pot or the substrate at the start of the irrigation cycle.
STRT_IRRIG.START_CAUSE | 665D | SUBSTR START | start cause 0=UNKNOWN 1=MANUAL 2=MOIST%-SLAB 3=DRY-OUT 4=RESTTIME 5=RADIATION SUM 6=EXTERNAL 7=DRAINAGE 8=SAFETY LEVEL |  | M500 The cause of every start.
STRT_IRRIG.START_NUM | 6661 | SUBSTR START | Cycle |  | M500 The sequence number of the irrigation cycle for this day.
IrrigatMeasCalc.CalcDryingInKg | 6644 | SUBSTR START | dry-out limit | kg | I500 I500 I500.2 M500
IrrigatMeasCalc.CalcTranspPerM2 | 67CE | SUBSTR START | transpiration rate | l/m²/hr | M500 The decrease in the measured humidity expressed in litres per m² per hour.
IrrigatMeasCalc.CurrentDesirWCon | 6653 | SUBSTR START | moisture level limit | % | I500 I500 I500.2 M500
IrrigatMeasCalc.CycleRadSum | 665A | SUBSTR START | radiation sum after last irrigation cycle | J/cm² | M500 The current measured radiation sum after the start of the last irrigation cycle
IrrigatMeasCalc.DampedTranspirat | 665E | SUBSTR START | Measured transpiration rate | ml/unit/h | I500
IrrigatMeasCalc.DesirDryoutUnit | 666C | SUBSTR START | dry-out limit | ml/unit | I500 I500 I500.2 M500
IrrigatMeasCalc.DesWghtUniInKg | 6678 | SUBSTR START | desired weight per unit | kg | M500
IrrigatMeasCalc.IrrigatPerState | 6689 | SUBSTR START | status 0=OFF 1=MANUAL 2=WAIT 3=NOT AVAILABLE 4=WAIT FOR TRANSPIR. 5=RAMPING 6=PERIOD RELEASE 7=FLUSHING RELEASED 8=IRRIGATION STOPPED 9=MIN START 10=END OF DAY 11=SAFETY START |  | I500 See 32 Period/status . M500 See 32 Period/status
IrrigatMeasCalc.MeasDryoutUnit | 669E | SUBSTR START | measured dry-out | ml/unit | I500 I500 I500.2 M500
IrrigatMeasCalc.MeasWContent | 66A2 | SUBSTR START | measured moisture level | % | I500 I500 I500.2 M500
IrrigatMeasCalc.MeasWghtTot | 66A8 | SUBSTR START | measured total weight | kg | I500 I500 I500.2 M500
IrrigatMeasCalc.MeasWghtUni | 66AA | SUBSTR START | measured weight per unit | kg/unit | M500
IrrigatMeasCalc.MinTranspStart | 66AD | SUBSTR START | transpiration rate limit | ml/unit/h | I500
IrrigatMeasCalc.SelMaxCycleRadSu | 66BB | SUBSTR START | radiation sum limit | J/cm² | M500 M500 The maximum radiation sum between the start of the last irrigation cycle and the start of the new irrigation cycle that is applicable for the current period.
IrrigatMeasCalc.UsedDrWghtTo_01 | 66D8 | SUBSTR START | Used saturation weight total | kg | I500 The total measured weight from the weighing scale at the last drain measurement (this value corresponds to the weight in M500.1).
ALG_POMP_.GER_POMPST | 4C4F | PUMP | Actual pump position 0=OFF 1=ON 2=LOW SP 3=HIGH SP |  | I350 Actual position of the transport pump, see 6 Actual pump position . M350 Actual position of the transport pump (only for switching pump).
ALG_POMP_.POMP_BEPERK | 4C51 | PUMP | Limitation pump drive 0=NONE 1=RELEASE 2=FIXED POS 3=MAX CAP 4=DEFECTIVE 5=EXT ERROR 6=CALIB ERROR 7=ALLOC INPUT 8=ALLOC OUTPUT 9=DRIVE 10=MEASUREMENT 11=HEAT SURP 12=TEMP 13=EXT DRIVE 14=NOT CONTROLLED 15=LOW TEMP HEAT SURP |  | I350 Indication of the limitation of the transport pump, see 10 Limitation pump drive . M350 Indication of the limitation of the transport pump.
TRANSCTL.GV_VERM_TOT | 4CE3 | TRANSP.MAIN | Des transport capacity | kW | M350 The required transport capacity that is passed on to the heat producers.
TRANSCTL.MK_TEMP_TOT | 4CE7 | TRANSP.MAIN | Desired transport temp | °C | M350 The desired temperature of the transport main from the heat management. The desired transport temperature is equal to the highest demanded water temperature from the connected compartments, heat block or combi block from the connected air treatment units plus the set Offset transport temperature .
TRANSSYS.GEM_TRAN_TEMP | 4CF0 | TRANSP.MAIN | measured supply temperature | °C | I350 M350
MomReserv.WProdBegr | 4F2E | MANIFOLD | total heat production limited | kW | M300.3
MomReserv.WProdOnbegr | 4F32 | MANIFOLD | total heat production unlimited | kW | M300.3
WARMTECTL.GEW_LOS_VERM | 4FC8 | MANIFOLD | Act capacity emptying | kW | M300 The capacity that the buffer supplies. This is calculated on the basis of the position of the off-take mixing valve. If the off-take mixing valve is open for 50%, then half of the demanded capacity from the greenhouse is supplied by the buffer.
WARMTECTL.GEW_TEMP | 4FC9 | MANIFOLD | total desired greenhouse temperature | °C | M300
WARMTECTL.GEW_VERM | 4FCA | MANIFOLD | total desired greenhouse capacity | kW | M300
MISTKLEP.GEW_CAP | 5009 | MIST VALVE | Calculated capacity | % | M180 Calculated capacity mist valve.
MISTKLEP.TOESTAND | 5010 | MIST VALVE | Status 0=NO RELEASE 1=WAIT PUMP 2=OFF 3=SPRAY PAUSE 4=SPRAY 5=PRESSURE RELIEF |  | I185 The status of the mist valve. M180 The status of the mist valve.
KASL_REF.REG_GEWAS_RV | 50B6 | HUMIDIF | Used relative humidity | % | I180.4 The humidity that is used for the humidification control.
KASL_REF.REG_GEWAS_TEMP | 50B7 | HUMIDIF | Measured temperature | °C | I180.4 The temperature that is used for the humidification control. M180 The measured temperature that is used for the misting control.
KASL_REF.REG_GEWAS_VD | 50B8 | HUMIDIF | Used humidity deficit | g/m³ | I180.4
VOCHT_CTL.BER_RV | 50EB | HUMIDIF | Calculated humidity limit | % | I180 The calculated humidity limit for switching the misting installation. I181 M180 The calculated humidity limit for switching the misting installation.
VOCHT_CTL.BER_VD | 50EC | HUMIDIF | Calculated humidity limit | g/m³ | I180 The calculated humidity limit for switching the misting installation. I181 M180 The calculated humidity limit for switching the misting installation.
VOCHT_CTL.GEM_RV | 50F2 | HUMIDIF | Measured humidity | % | M180 The measured air humidity that is used for the misting control.
VOCHT_CTL.GEWENSTE_TEMP | 50F5 | HUMIDIF | Calculated cooling temperature | °C | I180 I181 M180 The calculated cooling temperature for switching the misting installation.
VOCHT_CTL.INSTEL_TEMP | 50F9 | HUMIDIF | Set cooling temperature | °C | I180 M180 The set cooling temperature from I180 Misting/Strategy.
VOCHT_CTL.SETP_RV | 510D | HUMIDIF | Set humidity limit | % | M180 The set humidity limit from I180 Misting/Strategy.
VOCHT_CTL.SETP_VD | 5111 | HUMIDIF | Set humidity limit | g/m³ | M180 The set humidity limit from I180 Misting/Strategy.
BUFOPN.GEM_TEMP | 51D5 | SENSOR | Meas temperature buffer sensors | °C | M320
BUF_TOEST.LEGEN | 5206 | BUFFER | Emptying active 0=NO 1=YES |  | I320 Indication whether the emptying of the buffer is active. M300.1 Indication whether the emptying of the buffer is active. M320 Indication whether the emptying of the buffer is active.
BUF_TOEST.VULLEN | 5212 | BUFFER | Filling active 0=NO 1=YES |  | I320 Indication whether the filling of the buffer is active. M300.1 Indication whether the filling of the buffer is active. M320 Indication whether the filling of the buffer is active.
BUFFER.GEM_LTEMP_RET | 5223 | BUFFER | Measured return temperature emptying | °C | M320 The measured temperature of the return water from the compartments to the heat buffer during emptying. M325.1 The measured temperature of the return water from the compartment(s) to the heat buffer during emptying.
BUFFER.GEM_TEMP_AANV | 5225 | BUFFER | Measured supply temperature | °C | M320 The measured temperature of the supply water from the heat source(s) to the heat buffer(s) (during filling), or from the heat buffer to the compartments (when emptying). M325.1 The measured temperature of the supply water from the heat source(s) to the heat buffer(s) (during filling), or from the buffer to the compartments (when emptying).
BUFFER.GEM_VTEMP_RET | 5228 | BUFFER | Measured return temperature filling | °C | M320 The measured temperature of the return water from the heat buffer to the heat source(s) during filling. M325.1 The measured temperature of the return water from the heat buffer to the heat source(s) during filling.
BUFFER.GER_VUL_PERC | 5229 | BUFFER | Actual fill% | % | I320 Actual fill percentage. I320.1 The actual buffer filling percentage is calculated on the basis of the difference between the heat capacity that is loaded into the buffer and the heat capacity that is leaving the buffer at that instant. This percentage is limited between the minimum and maximum achievable filling percentage, determined on the basis of the measurements from the temperature sensors. M320 The actual fill percentage of the heat buffer.
BUFFER.GEW_VUL_PERC | 522C | BUFFER | Desired fill% | % | M320 The desired fill capacity of the heat buffer.
BUFFER.LEEG_BEPERK | 5230 | BUFFER | Limitation emptying 0=NONE 1=RELEASE 2=TOO COLD 3=EXT BLOCK 4=EMPTY 5=MIN FILL% 6=FILL |  | I320 Possible cause why the buffer is not being emptied. M300.1 The limitation why the buffer is not being emptied. M320 The limitation why the buffer is not being emptied.
BUFFER.VUL_BEPERK | 524A | BUFFER | Limitation filling 0=NONE 1=RELEASE 2=TEMP 3=FULL 4=MAX FILL% 5=EMPTYING |  | I320 Possible cause why the buffer is not being filled. M300.1 The limitation why the buffer is not being filled. M320 The limitation why the buffer is not being filled.
WARMW_TE_VM.GEW_KET_VERM | 52C5 | HEAT EXCH | desired greenhouse capacity | kW | M300 M340 The desired heat capacity that has been allocated to this heat exchanger because of a capacity demand from the compartments.
WARMWIS_ALG.BEPERKING_WW | 52CC | HEAT EXCH | limitation heat exchanger 0=NONE 1=MANUAL 2=MAX CAP 3=NO RELEASE 4=EXTERNAL 5=HX DISCONNECTED 6=ALLOC INPUT 7=ALLOC OUTPUT 8=CALIB SERVO 9=ALLOC SERVO 10=LIMIT SERVO 11=CONTROL SERVO 12=INPUT HX DEFECT 13=NO TEMP 14=TOO WARM 15=COOLING WATER |  | M300.1 See 14 Limitation HX M340
WARMWIS_ALG.BER_WW_TEMP | 52CE | HEAT EXCH | calculated heat exchangers temperature | °C | I340 M300.1 The calculated supply temperature of the heat exchanger. M340 The temperatures of the heat exchanger.
WARMWIS_ALG.GER_KET_TEMP | 52D6 | HEAT EXCH | heat exchangers temperature | °C | I340 M300.1 The measured supply temperature of the heat exchanger. M340 The temperatures of the heat exchanger.
WARMWIS_ALG.GER_KET_VERM | 52D8 | HEAT EXCH | actual capacity | kW | M300 M340
WARMWIS_ALG.GEW_OPSLAG_VERM | 52DC | HEAT EXCH | Des forced storage capacity | kW | I340.2 Desired capacity of the exchanger that is calculated for the filling of the heat buffer in the active period. See Gedwongen opslag in warmtebuffer. M300 M340 The desired storage capacity of the heat exchanger if the buffer strategy demands this (refer to I330.2 Heat power/Forced storage).
WARMWIS_ALG.GEW_RESERV_VERM | 52DD | HEAT EXCH | Des reserve capacity | kW | M300 M340 The desired reserve capacity of the heat exchanger if the heat reserve demands this. The heat reserve demands a capacity to meet an expected future heat demand.
WARMWIS_ALG.KET_VERN_VRIJG | 52E1 | HEAT EXCH | Heat surplus% | % | M300.1 The heat surplus percentage of the heat exchanger. If the heat exchanger becomes too hot due to a forced demand, the heat surplus percentage increases. M340 The heat surplus percentage of the heat exchanger.
WARMWIS_MEET.GEM_T_RET_WW | 5305 | HEAT EXCH | Measured return temperature | °C | M340 The measured return temperature of the heat exchanger.
WARMWIS_TOEST.TOESTAND | 5331 | HEAT EXCH | status heat exchanger 0=LIMITED 1=READY 2=PRE-RUN 3=POST RUNNING 4=MIN TIME ON 5=ON 6=ERROR |  | I340 Status of the heat exchanger M300.1 Indication of the status of the heat exchanger. See 13 Status HX M340 Indication of the status of the heat exchanger.
WARMWIS_VERM.GEW_WARM_VERM_W | 533D | HEAT EXCH | Des heating capacity | kW | M300 The total demanded heat capacity from the heat exchanger. M340 The desired heat capacity of the heat exchanger. This is the sum of the desired greenhouse capacity and the internal capacity.
WASROBOT.BEPERKING | 5352 | WASH ROBOT | Limitation 0=NONE 1=NO RELEASE 2=WIND 3=TEMP 4=WIND/TEMP 5=MAN OFF |  | I240 Present limitation of the wash robot. M240 See 12 Limitation .
WASROBOT.ROBOT_TOEST | 535C | WASH ROBOT | Status wash robot 0=OFF 1=REST 2=WAIT RELEASE 3=START 4=OPERATION 5=ERROR |  | I240 M240 See 11 Status wash robot .
FILTER.FILTER_BEPERK | 5395 | FILTER | filter limitation 0=NONE 1=CONSUMPTION MAX 2=CONSUMPTION MIN 3=START ERROR 4=EXT ERROR 5=DIRTY |  | M430.1 M431
FILTER.FILTER_TOESTAND | 5397 | FILTER | filter status 0=REST 1=RECIPE 2=START 3=CLEANING BACK W 4=ERROR 5=RINSE 6=OPERATION 7=O & CLEANING 8=LIMIT FLOW |  | M430 The status of the filter rinse. M430.1 M431
TEMP_M.GEM_TEMP | 5488 | WAT SYS | Measured water temperature | °C | I432 Temperature of the water of which the EC is measured. The EC depends on the temperature and must be corrected for this.
VialuxFlow.CalculatedFlow | 551F | UV SYSTEM | Calculated flow | m³/hr | M450
VialuxFlow.MeasuredFlow | 5601 | UV SYSTEM | Measured flow | m³/hr | M450
VialuxSystem.CalcUVdosage | 55CC | UV SYSTEM | Calculated UV | mJ/cm² | M430.1 M450 The calculated UV dosage.
VialuxSystem.Limitation | 65DC | UV SYSTEM | Limitation 0=NONE 1=CONTROL OFF 2=RELEASE SETTING 3=RELEASE EXTERNAL 4=UV DOSAGE 5=LAMP COOL DOWN 6=FLOW DEFECTIVE 7=CHAMBER HOT 8=FLOW TOO LOW 9=FLOW TOO HIGH 10=START UV 11=DOS TOO LOW 12=LAMP OFF 16=WIPER OUT 17=WIPER IN 18=WIPER MOTOR 19=WIPER CONTACT 20=ERROR 21=I UV SENSOR 22=I WIPER OUT 23=I WIPER HOME 24=I WIPER CTL 25=I WIPER THERM 26=I V5 DISINFECTED 27=I ERROR 28=I RELEASE 29=I ACID TANK 30=I TEMP 31=I LAMP 35=EXPOSURE TIME 36=WIPER MAN OPER 37=WIPER HOME ER 38=V5 DISINFECTED 39=T10 TOO LOW 40=I POWER FAILURE 41=POWER FAILURE 50=TRANSLUCENCY 51=PEROXIDE 52=ACID 53=TYPE UV CHAMBER 54=DISINFECT 55=PURIFY 56=CONFIGURATION 57=ACID RINSE 58=PUMP OFF 59=DOSAGE 60=I V5 PURIFIED 61=V5 PURIFIED |  | I453 The limitation of the UV system. See Limitation. M430.1 M450
VialuxSystem.MeasUVdosage | 55B4 | UV SYSTEM | UV dos. | mJ/cm² | M430.1 M450 The measured UV dosage that has been calculated from the measured intensity (measured by the UV sensor) and the measured flow. This means it is a good measurement for the UV dosage.
VialuxSystem.ProcessState | 55EA | UV SYSTEM | Status 0=REST 1=START 2=PRODUCTION 3=ACID RINSE 4=ERROR 5=POST RUNNING |  | I453 The status of the UV system. See Status . M430.1 M450 The status of the UV system.
VialuxSystem.StatusLamps | 5555 | UV SYSTEM | Lamp status 0=OFF 1=LOW 2=MID 3=HIGH 4=COOL DOWN |  | I453 The status of the lamp. M450 The status of the lamp: OFF, LOW, MIDDLE, HIGH or COOL DOWN.
VialuxSystem.Translucency | 55BF | UV SYSTEM | Translucency | % | M450 The translucency indicates the level of the measured UV-C intensity in respect of the measured UV-C intensity of a cleaned tube.
DOS_CTL.BEPERKING | 5660 | WAT SYS | dosage limitation 0=NONE 1=CHANNEL 2=MIXING TANK 3=EXTERNAL 4=pH CALIB 5=ECs SNS 6=EC SNS 7=pH SNS 8=CTR pH ↓ 9=CTR pH ↑ 10=CTR EC ↑ 11=CTR EC ↓ 12=RCP pH ↓ 13=RCP pH ↑ 14=RCP EC ↑ 15=RCP EC ↓ 16=FINE TUNING 17=NUTRONIC 18=CONNECTION |  | M420 M430.1
DOS_CTL.TOESTAND | 5665 | WAT SYS | dosage status 0=REST 1=CHECK 2=START 3=OPERATION 4=RESET 5=ERROR 6=NUTRONIC |  | I420 Status of the dosage. M420 M430 The status of the dosage. M430.1
DOS_EC_CTL.REGEL_EC | 5667 | WAT SYS | calculated EC | mS/cm | M420 M430.1
DOS_PH_CTL.REGEL_PH | 5669 | WAT SYS | calculated pH | pH | M420 M430.1
EC_BOX.GEM_EC | 56A9 | WAT SYS | EC | mS/cm | M420 M430 The measured EC value. M430.1
EC_M_SENSOR.GEM_EC | 56AE | WAT SYS | EC supply | mS/cm | M420 M430 The measured EC value of the supply water. M430.1 The measured EC value of the supply water.
EC_VR.BER_EC_VR | 56B2 | WAT SYS | calculated EC supply | mS/cm | M420 M430.1 The calculated EC value of the supply water.
GIETWVER.GEM_TEMP | 5709 | WAT SYS | irrigation water temperature | °C | I423 Temperature of the irrigation water. M420 M430 The temperature of the irrigation water. M430.1
PH_BOX.GEM_PH | 5752 | WAT SYS | pH | pH | M420 M430 The measured pH value. M430.1
VialuxCascade.CascadeActCap | 577B | WAT SYS | Actual capacity | m³/hr | I453
VialuxCascade.CascadeDesireCap | 577D | WAT SYS | Desired capacity | m³/hr | I453 The desired capacity of the UV systems.
WATDIS.BEPERKING | 5787 | WAT SYS | water system limitation 0=NONE 7=DOSAGE 8=IRR W HEAT 9=EC SUPPLY 10=WATER MIX 11=SYST PUMP 12=CONSUMP 13=SET WAIT 14=EXT WAIT 15=UV SYSTEM 41=RETURN 42=DESTINATION TANK 43=RECYCLE TANK 44=FRESH WATER TANK 45=OVER DEM 46=MAX CAPACITY 47=VALVE GROUP CHANGE 48=RECIPE CHANGE 49=RINSE VALVE CHANGE 50=EXTERN WATER TR. 51=RETURN PIT ON MAX |  | I430 Limitation of the water system. M430.1
WATDIS.BER_FLOW | 5788 | WAT SYS | calculated flow | m³/hr | M420 M430 The expected flow is determined by the total capacity of all active valves of the water system. M430.1
WATDIS.FLOW | 578E | WAT SYS | water flow water irrigation | m³/hr | M420 M430 The measured flow for the irrigation. M430.1
WATDIS.RECEPT_NR | 579A | WAT SYS | recipe |  | M430 The recipe number that is presently active, or the recipe that was used during the last irrigation cycle. M430.1
WATDIS.TOESTAND | 57A5 | WAT SYS | water system status 0=REST 1=CHECK 2=PRE-RUN 3=OPERATION 4=ERROR 5=WAIT 6=FILTER 7=UV SYSTEM 8=BLOCKED |  | I430 Status of the water system. M430 See: I430 Storing watersysteem/Reset & halt. M430.1 M440 The status of the water system.
CO2wk_Prod.CdactBer | 5821 | CHP | CO₂ production active 0=NO 1=YES |  | M250 M330.1 Indication whether there is CO2 dosage with the CHP.
VERM_M_UI.VE_GEM | 58D8 | CHP | Measured electr. capacity | kW | M200 The actual electrical capacity of the CHP, which is determined by measuring the electrical production.
WK_ELB.AAN_VERM_BRON | 58E1 | CHP | Electrical capacity on | kW | M200 Capacity limit above which the CHP is activated for electricity demand. Even if the CHP is already active for a heat, CO₂ or storage demand, the electricity demand on the CHP must be greater than this limit before the CHP can start to supply electricity to the management. The lighting system can only be switched on after this.
WK_ELB.BEPERKING | 58E5 | CHP | Limitation 0=NONE 1=BLOCK 2=RELEASE 3=CHP 4=MAX GAS 5=STRATEGY 6=UNBALANCED OFF 7=COOLING WATER 8=ELECTR.PROD |  | M200
WK_ELB.BRON_PRODUCEERT | 58E8 | CHP | Electricity production active 0=NO 1=YES |  | M200 Indication whether the electricity production by the CHP is active.
WK_ELB.GER_CAP_BRON | 58F2 | CHP | Max electrical capacity | kW | M200 The maximum electrical capacity to be supplied by the CHP.
WK_ELB.GEW_EXTERN_AAN | 58F3 | CHP | Des electrical capacity | kW | M300 The desired electrical capacity of the CHP, determined by an electricity demand from the electricity management. M330 The desired electrical capacity for the CHP, determined by an electricity demand from the electricity management.
WK_ELB.VE_WK_VOLBESCH | 5900 | CHP | actual electricity capacity CHP fully available | kW | M200 If the measured actual capacity (see Act electrical capacity ) rises above the limit shown here, the CHP is fully available to supply electricity to the electricity consumers such as lighting systems and electrical consumers.
WK_SYS.BEPERKING | 590C | CHP | limitation CHP 0=NONE 1=TOO WARM 2=ERROR 3=RELEASE 4=NOT AVAILABLE 5=MANUAL 6=MAX GAS 7=UNBALANCED OFF 8=COOLING WATER 9=PART LOAD 10=ELECTR. RELEASE |  | I330 The limitation of the CHP, see M330 Warmtekracht/Overzicht. M250.1 Report of the limitation of the CHP. See M300.1 HT-warmtebeheer - HT-bronnen. M300.1 The limitation of the CHP. M330 The limitation of the CHP.
WK_SYS.GEM_AANV_TEMP | 5918 | CHP | measured supply temperature | °C | M300.1 The measured supply temperature of the CHP. M330
WK_SYS.GEM_RET_TEMP | 5919 | CHP | measured return temperature | °C | M300.1 The measured return temperature of the CHP. M330
WK_SYS.GER_KET_VERM | 591B | CHP | CHP heat capacity control | kW | I330 Actual heat power by the CHP. M300 M330 M330 The actual heat capacity from this CHP.
WK_SYS.GEW_EXTERN_VERM | 591C | CHP | Des external capacity | kW | I330.1 Desired external capacity demand to the CHP. M300 The desired capacity when the CHP is controlled to switch on because of an external demand (for example an external electricity demand). M330 The desired capacity when the CHP is controlled because of an external demand (for example an external electricity demand).
WK_SYS.GEW_OPSLAG_VERM | 591F | CHP | Des forced storage capacity | kW | I330.2 Desired capacity of the CHP that is calculated for the filling of the heat buffer in the active period. See Gedwongen opslag in warmtebuffer. M300 M330 The desired capacity of the CHP if the buffer strategy demands this (refer to I330.2 Heat power/Forced storage).
WK_SYS.KET_VERN_VRIJG | 5921 | CHP | Heat surplus% | % | M300.1 The heat surplus percentage of the heat exchanger. If the heat exchanger becomes too hot due to a forced demand, the heat surplus percentage increases. M330 The heat surplus percentage that is present with this CHP.
WK_SYS.TOESTAND | 5931 | CHP | status CHP 0=OFF 1=ON 2=MIN TIME OFF 3=MIN TIME ON 4=DELAY OFF 5=DELAY NEXT ON 6=DELAY NEXT OFF 7=TOO COLD 9=DELAY ON |  | I330 The status of the CHP, see M330 Warmtekracht/Overzicht. M250.1 M300.1 Indication of the status of the CHP. M330 Indication of the status of the CHP.
WK_SYS.WK_EXT_BLOK_ACT | 593B | CHP | External blocking 0=NO 1=YES |  | M330 Indication that the external blocking is active.
WK_SYSTEEM.GEW_CO2_VERM | 594A | CHP | desired CO₂ capacity | kW | M300 The desired CO2 capacity of the CHP. M330 The desired CO2 capacity for the CHP, because of a demand to CO2 from the CO2 management.
WK_SYSTEEM.GEW_CONS_VERM | 594B | CHP | desired greenhouse capacity | kW | M300 M330 The desired heat capacity that has been allocated to this CHP because of a capacity demand from the compartments.
WK_SYSTEEM.GEW_RESERV_VERM | 594E | CHP | Des reserve capacity | kW | M300 M330 The desired reserve capacity of the CHP if the heat reserve demands this. The heat reserve demands a capacity to meet the expected future heat demand.
Lichtuitstoot.Percentage | 5A8F |  | Calculated maximum light emission | % | I207 Maximum permitted light emission. Dependent on the I168 Curtain/Control setting, line 17: Light emission: min. curtain position the curtain is controlled to a minimum curtain position.